<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.04" y2="0" width="0" layer="20"/>
<wire x1="39.04" y1="0" x2="39.04" y2="19.04" width="0" layer="20"/>
<wire x1="39.04" y1="19.04" x2="0" y2="19.04" width="0.3048" layer="20"/>
<wire x1="0" y1="19.04" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<description>&lt;b&gt;FabAcademy Library&lt;/b&gt;</description>
<packages>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="OP1206">
</package>
</packages>
</library>
<library name="Working">
<packages>
<package name="R1206FAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED" library="fab" package="LED1206FAB" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Working" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Working" package="R1206FAB" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Working" package="R1206FAB" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="SOIC8" value="ATTINY45SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="Q1" library="fab" package="OP1206" value="PHOTOTRANSISTOR-NPN1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$3" pad="1"/>
<contactref element="Q1" pad="EMITTER"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="MISO_PB1">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="SCK_PB2">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="MOSI_PB0">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="5"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="PB3">
<contactref element="U$1" pad="2"/>
<contactref element="Q1" pad="COLLECTOR"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U$1" pad="3"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="LED" pad="2"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
