<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.085" y2="0" width="0.4064" layer="20"/>
<wire x1="45.085" y1="0" x2="45.085" y2="26.67" width="0.4064" layer="20"/>
<wire x1="45.085" y1="26.67" x2="0" y2="26.67" width="0.4064" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<description>&lt;b&gt;FabAcademy Library&lt;/b&gt;</description>
<packages>
<package name="C1206FAB">
</package>
<package name="2X02SMD">
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
<library name="rodney">
<description>&lt;B&gt;My Personal Library&lt;/B&gt;
&lt;p&gt;Created: 18 Apr 2015&lt;/p&gt;
&lt;p&gt;Owner: Rodney Dorville&lt;/p&gt;</description>
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="I2C" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="ISP" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="LED" library="fab" package="LED1206FAB" value="RED"/>
<element name="R1" library="fab" package="R1206FAB" value="10K"/>
<element name="R2" library="fab" package="R1206FAB" value="499"/>
<element name="R3" library="fab" package="R1206FAB" value="10K"/>
<element name="R4" library="fab" package="R1206FAB" value="10K"/>
<element name="FTDI" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U1" library="rodney" package="SOIC8" value="ATTiny45"/>
</elements>
<signals>
<signal name="MISO">
<contactref element="ISP" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="I2C" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="RST">
<contactref element="ISP" pad="5"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="ISP" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="FTDI" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="I2C" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="I2C" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="ISP" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="FTDI" pad="1"/>
<contactref element="I2C" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="LED" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="FTDI" pad="5"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="TXD">
<contactref element="FTDI" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
