<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_fab">
<packages>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="ModernDevice">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="SMT_PINS_2">
</package>
<package name="SMT_PINS_4">
</package>
</packages>
</library>
<library name="01_battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AB9V">
<description>&lt;B&gt;9-V BATTERY CLIP&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="16MHZ" library="01_fab" package="EFOBM" value="RESONATOR"/>
<element name="C1" library="01_SparkFun" package="1206" value="100uF"/>
<element name="C2" library="01_SparkFun" package="1206" value="10uF"/>
<element name="C3" library="01_SparkFun" package="1206" value="1000uF"/>
<element name="C4" library="01_SparkFun" package="1206" value=".1uF"/>
<element name="CVR" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="G1" library="01_battery" package="AB9V" value="AB9V"/>
<element name="G2" library="01_battery" package="AB9V" value="5V"/>
<element name="JP1" library="01_FAB_Hello" package="2X03SMD" value=""/>
<element name="PG1" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG2" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG3" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG4" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG5" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG6" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG7" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="PG8" library="01_ng" package="SMT_PINS_2" value="2_PIN_HEADERHEADER"/>
<element name="R1" library="01_SparkFun" package="1206" value="10K"/>
<element name="R10" library="01_SparkFun" package="1206" value="499"/>
<element name="R11" library="01_SparkFun" package="1206" value="10K"/>
<element name="R12" library="01_SparkFun" package="1206" value="10K"/>
<element name="R13" library="01_SparkFun" package="1206" value="0ohm"/>
<element name="R2" library="01_SparkFun" package="1206" value="10K"/>
<element name="R3" library="01_SparkFun" package="1206" value="10K"/>
<element name="R4" library="01_SparkFun" package="1206" value="10K"/>
<element name="R5" library="01_SparkFun" package="1206" value="10K"/>
<element name="R6" library="01_SparkFun" package="1206" value="10K"/>
<element name="R7" library="01_SparkFun" package="1206" value="10K"/>
<element name="R8" library="01_SparkFun" package="1206" value="10K"/>
<element name="R9" library="01_SparkFun" package="1206" value="499"/>
<element name="RGB12" library="01_ng" package="SMT_PINS_4" value=""/>
<element name="RGB16" library="01_ng" package="SMT_PINS_4" value=""/>
<element name="U1" library="ModernDevice" package="TQFP32-08" value="ATMEGA328"/>
<element name="U$1" library="01_SparkFun" package="SOT23-3" value="LM3480IM4"/>
<element name="R14" library="01_SparkFun" package="1206" value="0Ohm"/>
<element name="R15" library="01_SparkFun" package="1206" value="0ohm"/>
</elements>
<signals>
<signal name="GND">
<contactref element="16MHZ" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="CVR" pad="1"/>
<contactref element="PG8" pad="1"/>
<contactref element="PG7" pad="1"/>
<contactref element="PG6" pad="1"/>
<contactref element="PG5" pad="1"/>
<contactref element="PG4" pad="1"/>
<contactref element="PG3" pad="1"/>
<contactref element="PG2" pad="1"/>
<contactref element="PG1" pad="1"/>
<contactref element="RGB12" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="RGB16" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="G2" pad="-"/>
<contactref element="R13" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="G1" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="PG1IN">
<contactref element="PG1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="PG2IN">
<contactref element="PG2" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="PG3IN">
<contactref element="PG3" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="PG4IN">
<contactref element="PG4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="14"/>
</signal>
<signal name="PG5IN">
<contactref element="PG5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="PG6IN">
<contactref element="PG6" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="PG7IN">
<contactref element="PG7" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="PG8IN">
<contactref element="PG8" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="N$27">
<contactref element="U1" pad="31"/>
</signal>
<signal name="N$28">
<contactref element="U1" pad="30"/>
</signal>
<signal name="N$30">
<contactref element="U1" pad="20"/>
</signal>
<signal name="N$32">
<contactref element="16MHZ" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="16MHZ">
<contactref element="16MHZ" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="CVR_IN">
<contactref element="U1" pad="22"/>
<contactref element="CVR" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="DO2">
<contactref element="U1" pad="12"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="DO1">
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="N$1">
<contactref element="R9" pad="2"/>
<contactref element="RGB12" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R10" pad="2"/>
<contactref element="RGB16" pad="3"/>
</signal>
<signal name="5V">
<contactref element="RGB16" pad="1"/>
<contactref element="RGB12" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="G2" pad="+"/>
</signal>
<signal name="9V">
<contactref element="U$1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="G1" pad="+"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
