<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="PANASONIC_D">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="01_battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AB9V">
<description>&lt;B&gt;9-V BATTERY CLIP&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="01_atmega8">
<description>&lt;b&gt;Atmel ATmega8, ATmega48, ATmega88, ATmega168: 8-bit AVR microcontrollers&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;ATmega8, ATmega8L:&lt;br&gt;
28-pin PDIP, 32-lead TQFP and 32-pad QFN/MLF
&lt;li&gt;ATmega48, ATmega48V, ATmega88, ATmega88V, ATmega168, ATmega168V:&lt;br&gt;
 28-pin PDIP, 32-lead TQFP and 32-pad QFN/MLF (no 28-pad QFN/MLF!)
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="ESP8266">
<packages>
<package name="ESP-01">
</package>
</packages>
</library>
<library name="ModernDevice">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="01_SparkFun" package="1206" value="100uf"/>
<element name="C3" library="01_FAB_Hello" package="1206" value=".1uf"/>
<element name="CLOCK" library="01_fab" package="EFOBM" value="16MHz"/>
<element name="G1" library="01_battery" package="AB9V" value="AB9V"/>
<element name="IC1" library="01_atmega8" package="TQFP32-08" value="ATMEGA48/88/168-AU"/>
<element name="JP1" library="01_FAB_Hello" package="2X03SMD" value=""/>
<element name="R1" library="01_FAB_Hello" package="1206" value="1K"/>
<element name="R2" library="01_FAB_Hello" package="1206" value="1K"/>
<element name="R3" library="01_FAB_Hello" package="1206" value="1K"/>
<element name="R4" library="01_FAB_Hello" package="1206" value="1K"/>
<element name="R5" library="01_FAB_Hello" package="1206" value="10K"/>
<element name="R7" library="01_SparkFun" package="1206" value="0ohm"/>
<element name="R8" library="01_SparkFun" package="1206" value="0ohm"/>
<element name="U$3" library="ESP8266" package="ESP-01" value="ESP8266-01"/>
<element name="U1" library="ModernDevice" package="SOT23-5" value="V_REG_LDOSMD"/>
<element name="R6" library="01_SparkFun" package="1206" value="0ohm"/>
<element name="R9" library="01_SparkFun" package="1206" value="0ohm"/>
<element name="R10" library="01_SparkFun" package="1206" value="0ohm"/>
<element name="C5" library="01_SparkFun" package="PANASONIC_D" value="100uf"/>
<element name="C6" library="01_SparkFun" package="PANASONIC_D" value="100uf"/>
</elements>
<signals>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="29"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="U$3" pad="P$8"/>
<contactref element="CLOCK" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="21"/>
<contactref element="U1" pad="2"/>
<contactref element="G1" pad="-"/>
<contactref element="C5" pad="-"/>
<contactref element="C6" pad="-"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC1" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C6" pad="+"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="12"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="13"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="U$3" pad="P$3"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="2"/>
<contactref element="U$3" pad="P$2"/>
</signal>
<signal name="RX">
<contactref element="U$3" pad="P$5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="TX">
<contactref element="U$3" pad="P$1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="7"/>
<contactref element="CLOCK" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="8"/>
<contactref element="CLOCK" pad="3"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$4">
</signal>
<signal name="9V">
<contactref element="G1" pad="+"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="C5" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
