<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="53.34" y1="48.26" x2="98.73" y2="48.26" width="0" layer="20"/>
<wire x1="98.73" y1="48.26" x2="98.73" y2="72.38" width="0" layer="20"/>
<wire x1="98.73" y1="72.38" x2="53.34" y2="72.38" width="0" layer="20"/>
<wire x1="53.34" y1="72.38" x2="53.34" y2="48.26" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="000_epi">
<packages>
<package name="ACELEROMETRO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_ng" package="1206" value="0.1uF"/>
<element name="C2" library="01_ng" package="1206" value="0.1uF"/>
<element name="C3" library="01_ng" package="1206" value="0.1uF"/>
<element name="C4" library="01_ng" package="1206" value="0.1uF"/>
<element name="JP1" library="01_SparkFun" package="1X06-SMD" value=""/>
<element name="IC1" library="000_epi" package="ACELEROMETRO" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="P14"/>
<contactref element="IC1" pad="P15"/>
</signal>
<signal name="XOUT">
<contactref element="JP1" pad="5"/>
<contactref element="IC1" pad="P12"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="ST">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="P2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC1" pad="P3"/>
<contactref element="IC1" pad="P5"/>
<contactref element="IC1" pad="P6"/>
<contactref element="IC1" pad="P7"/>
</signal>
<signal name="ZOUT">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="P8"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="YOUT">
<contactref element="JP1" pad="4"/>
<contactref element="IC1" pad="P10"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
