<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="44.45" width="0.254" layer="20"/>
<wire x1="0" y1="44.45" x2="55.88" y2="44.45" width="0.254" layer="20"/>
<wire x1="55.88" y1="44.45" x2="55.88" y2="0" width="0.254" layer="20"/>
<wire x1="55.88" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>RDuino</text>
</plain>
<libraries>
<library name="atmega8">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="fab">
<description>&lt;b&gt;FabAcademy Library&lt;/b&gt;</description>
<packages>
<package name="EFOBM">
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="Working">
<packages>
<package name="1X08_SMD_STRAIGHT_ALT">
</package>
<package name="1X10_SMD_STRAIGHT_ALT">
</package>
<package name="1X02_SMD_FLAT_PADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MICRO" library="atmega8" package="TQFP32-08" value="ATMEGA328P-AU">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="01_SparkFun" package="1206" value="10k"/>
<element name="SW1" library="01_FAB_Hello" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="01_FAB_Hello" package="1206" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="01_SparkFun" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="01_SparkFun" package="1206" value="1uF"/>
<element name="C5" library="01_SparkFun" package="1206" value="100pF"/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="H4" library="fab" package="2X03SMD" value="2X3"/>
<element name="H1" library="Working" package="1X10_SMD_STRAIGHT_ALT" value="1X10"/>
<element name="H2" library="Working" package="1X08_SMD_STRAIGHT_ALT" value="1X8"/>
<element name="H3" library="Working" package="1X08_SMD_STRAIGHT_ALT" value="1X8"/>
<element name="H5" library="Working" package="1X02_SMD_FLAT_PADS" value="M02"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="MICRO" pad="4"/>
<contactref element="MICRO" pad="6"/>
<contactref element="MICRO" pad="18"/>
<contactref element="MICRO" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="H4" pad="2"/>
<contactref element="LED" pad="1"/>
<contactref element="H5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="MICRO" pad="3"/>
<contactref element="MICRO" pad="5"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="MICRO" pad="21"/>
<contactref element="R2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="H4" pad="6"/>
<contactref element="H1" pad="10"/>
<contactref element="H3" pad="2"/>
<contactref element="H3" pad="1"/>
<contactref element="H5" pad="2"/>
</signal>
<signal name="RST">
<contactref element="MICRO" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="H4" pad="5"/>
<contactref element="H3" pad="8"/>
</signal>
<signal name="PD5">
<contactref element="MICRO" pad="9"/>
<contactref element="H1" pad="9"/>
</signal>
<signal name="PD6">
<contactref element="MICRO" pad="10"/>
<contactref element="H1" pad="8"/>
</signal>
<signal name="PD7">
<contactref element="MICRO" pad="11"/>
<contactref element="H1" pad="7"/>
</signal>
<signal name="PB0">
<contactref element="MICRO" pad="12"/>
<contactref element="H1" pad="6"/>
</signal>
<signal name="PB1">
<contactref element="MICRO" pad="13"/>
<contactref element="H1" pad="5"/>
</signal>
<signal name="PB2">
<contactref element="MICRO" pad="14"/>
<contactref element="H1" pad="4"/>
</signal>
<signal name="PB3_MOSI">
<contactref element="MICRO" pad="15"/>
<contactref element="H4" pad="4"/>
<contactref element="H1" pad="3"/>
</signal>
<signal name="PB4_MISO">
<contactref element="MICRO" pad="16"/>
<contactref element="H4" pad="1"/>
<contactref element="H1" pad="2"/>
</signal>
<signal name="PD0_RXD">
<contactref element="MICRO" pad="30"/>
<contactref element="H3" pad="7"/>
</signal>
<signal name="PD1_TXD">
<contactref element="MICRO" pad="31"/>
<contactref element="H3" pad="6"/>
</signal>
<signal name="PD2_INT0">
<contactref element="MICRO" pad="32"/>
<contactref element="H3" pad="5"/>
</signal>
<signal name="PD3_INT1">
<contactref element="MICRO" pad="1"/>
<contactref element="H3" pad="4"/>
</signal>
<signal name="ADC6">
<contactref element="MICRO" pad="19"/>
<contactref element="H2" pad="8"/>
</signal>
<signal name="ADC7">
<contactref element="MICRO" pad="22"/>
<contactref element="H2" pad="7"/>
</signal>
<signal name="PC0">
<contactref element="MICRO" pad="23"/>
<contactref element="H2" pad="6"/>
</signal>
<signal name="PC1">
<contactref element="MICRO" pad="24"/>
<contactref element="H2" pad="5"/>
</signal>
<signal name="PC2">
<contactref element="MICRO" pad="25"/>
<contactref element="H2" pad="4"/>
</signal>
<signal name="PC3">
<contactref element="MICRO" pad="26"/>
<contactref element="H2" pad="3"/>
</signal>
<signal name="PC4_SDA">
<contactref element="MICRO" pad="27"/>
<contactref element="H2" pad="2"/>
</signal>
<signal name="PC5_SCL">
<contactref element="MICRO" pad="28"/>
<contactref element="H2" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="LED" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PB5_SCK">
<contactref element="MICRO" pad="17"/>
<contactref element="H4" pad="3"/>
<contactref element="H1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="3"/>
<contactref element="MICRO" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="MICRO" pad="7"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="PD4">
<contactref element="MICRO" pad="2"/>
<contactref element="H3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
