<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="18.415" y1="22.225" x2="67.615" y2="22.225" width="0" layer="20"/>
<wire x1="67.615" y1="22.225" x2="67.615" y2="44.44" width="0" layer="20"/>
<wire x1="67.615" y1="44.44" x2="18.415" y2="44.44" width="0" layer="20"/>
<wire x1="18.415" y1="44.44" x2="18.415" y2="22.225" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="A3216-18">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SMT_PINS_3">
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="01_ng" package="A3216-18" value=""/>
<element name="JP1" library="01_SparkFun" package="1X06-SMD" value=""/>
<element name="R1" library="01_ng" package="1206" value=""/>
<element name="U$1" library="01_SparkFun" package="SO08-EIAJ" value="ATTINY45"/>
<element name="U$2" library="01_FAB_Hello" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$4" library="01_ng" package="SMT_PINS_3" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$2" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="8"/>
<contactref element="C1" pad="+"/>
<contactref element="R1" pad="2"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="6"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="-"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="CTS">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="RTS">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="2"/>
<contactref element="U$4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
