int led = 10;

// the setup routine runs once when you press reset:

void setup() {

// initialize the digital pin as an output.

pinMode(PA3, OUTPUT);

}

// the loop routine runs over and over again forever:

void loop() {

digitalWrite(PA3, HIGH);

// Port A P3 is High (HIGH is the voltage level)

}