int led = 10;

// the setup routine runs once when you press reset:

void setup() {

 // initialize the digital pin as an output.

 pinMode(PA3, OUTPUT);

}

// the loop routine runs over and over again forever:

void loop() {

 digitalWrite(PA3, HIGH);

 // Port A P3 is High (HIGH is the voltage level)

}