<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.15" y2="0" width="0" layer="20"/>
<wire x1="30.15" y1="0" x2="30.15" y2="17.77" width="0" layer="20"/>
<wire x1="30.15" y1="17.77" x2="0" y2="17.77" width="0" layer="20"/>
<wire x1="0" y1="17.77" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_adafruit">
<packages>
<package name="1X08-BIG">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="SCREW_2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="01_adafruit" package="1X08-BIG" value=""/>
<element name="U$1" library="01_ng" package="SCREW_2" value="2_PIN_HEADERSCREW"/>
<element name="U$2" library="01_ng" package="SCREW_2" value="2_PIN_HEADERSCREW"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$2" pad="2"/>
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="7"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
