<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="67.564" y1="38.227" x2="67.183" y2="2.397" width="0.254" layer="20"/>
<wire x1="67.183" y1="2.397" x2="65.929" y2="-1.651" width="0.254" layer="20" curve="-90"/>
<wire x1="65.929" y1="-1.651" x2="6.334" y2="-1.397" width="0.254" layer="20"/>
<wire x1="6.334" y1="-1.397" x2="3.683" y2="1.254" width="0.254" layer="20" curve="-90"/>
<wire x1="3.683" y1="1.254" x2="3.683" y2="52.594" width="0.254" layer="20"/>
<wire x1="3.683" y1="52.594" x2="6.08" y2="58.039" width="0.254" layer="20" curve="-90"/>
<wire x1="6.08" y1="58.039" x2="67.564" y2="58.039" width="0.254" layer="20"/>
<wire x1="67.564" y1="58.039" x2="67.564" y2="38.227" width="0.254" layer="20"/>
<text>DIGITAL</text>
<text>GND</text>
<text>5V Gnd 12V</text>
<text>0 1 2 3 4 5</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>AREF</text>
<text>3V3</text>
<text>RES</text>
<text>USB</text>
<text>ETH</text>
<text>DIGITAL</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>ANALOG</text>
<text>RST</text>
<text>3.3V</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>VIN</text>
<text>IOREF</text>
<text>SCL</text>
<text>SDA</text>
<text>AREF</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
</plain>
<libraries>
<library name="pinhead">
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SmartPrj">
<packages>
<package name="1X08-TH">
</package>
<package name="1X10-TH">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="PAD.1">
</package>
</packages>
</library>
<library name="CopyHelper">
<packages>
<package name="TO92">
</package>
</packages>
</library>
<library name="uln-udn">
<description>&lt;b&gt;Driver Arrays&lt;/b&gt;&lt;p&gt;
ULN and UDN Series&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X07">
</package>
<package name="1X05">
</package>
<package name="1X02">
</package>
<package name="1X02_BIG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PINS8-SCL" library="SmartPrj" package="1X10-TH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PINS0-7" library="SmartPrj" package="1X08-TH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANALOG" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="SmartPrj" package="1X08-TH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="01_ng" package="PAD.1" value=""/>
<element name="STAB" library="CopyHelper" package="TO92" value="">
<attribute name="PACKAGE" value="TO-92"/>
<attribute name="CURRENT" value="0.1 A"/>
<attribute name="VIN-MIN" value="5.0 V"/>
<attribute name="MANUFACTURER" value="St Microelectronics"/>
<attribute name="TME" value="L78L33ACZ"/>
<attribute name="VIN-MAX" value="30.0 V"/>
<attribute name="VOUT" value="3.3 V"/>
</element>
<element name="DRIVER" library="uln-udn" package="DIL16" value="ULN2003AN"/>
<element name="RFID" library="SparkFun-Connectors" package="1X07" value=""/>
<element name="MOTOR" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="BUTTON" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X02_BIG" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="PINS8-SCL" pad="1"/>
<contactref element="RFID" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="RFID" pad="7"/>
<contactref element="POWER" pad="4"/>
</signal>
<signal name="GND">
<contactref element="RFID" pad="5"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="POWER" pad="7"/>
<contactref element="POWER" pad="6"/>
<contactref element="STAB" pad="2"/>
<contactref element="DRIVER" pad="8"/>
<contactref element="BUTTON" pad="2"/>
</signal>
<signal name="0">
<contactref element="PINS8-SCL" pad="3"/>
<contactref element="JP2" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="DRIVER" pad="16"/>
<contactref element="MOTOR" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="DRIVER" pad="15"/>
<contactref element="MOTOR" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="DRIVER" pad="14"/>
<contactref element="MOTOR" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="DRIVER" pad="13"/>
<contactref element="MOTOR" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="MOTOR" pad="5"/>
<contactref element="DRIVER" pad="9"/>
<contactref element="STAB" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="STAB" pad="3"/>
<contactref element="POWER" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="RFID" pad="2"/>
<contactref element="PINS8-SCL" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="RFID" pad="3"/>
<contactref element="PINS8-SCL" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="RFID" pad="4"/>
<contactref element="PINS8-SCL" pad="5"/>
</signal>
<signal name="N$14">
<contactref element="BUTTON" pad="1"/>
<contactref element="PINS8-SCL" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="PINS0-7" pad="8"/>
<contactref element="DRIVER" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="DRIVER" pad="3"/>
<contactref element="PINS0-7" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="PINS0-7" pad="6"/>
<contactref element="DRIVER" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="DRIVER" pad="1"/>
<contactref element="PINS0-7" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="RFID" pad="1"/>
<contactref element="JP2" pad="P$2"/>
</signal>
<signal name="N$19">
</signal>
<signal name="N$3">
<contactref element="JP1" pad="1"/>
<contactref element="PINS0-7" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="PINS0-7" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
