<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="47.2948" x2="40.0304" y2="47.2948" width="0" layer="20"/>
<wire x1="40.0304" y1="47.2948" x2="40.0304" y2="0" width="0" layer="20"/>
<wire x1="40.0304" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="47.2948" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-lstb">
<packages>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="1X02_LONGPADS">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SV2" library="con-lstb" package="MA08-1" value=""/>
<element name="SV4" library="con-lstb" package="MA08-1" value=""/>
<element name="SV1" library="con-lstb" package="MA08-1" value=""/>
<element name="U$1" library="01_SparkFun" package="SO08" value="MOSFET-NCHANNEL-SOIC8"/>
<element name="MOTOR" library="01_SparkFun" package="1X02_LONGPADS" value="DC"/>
<element name="BATTERY" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="U$3" library="01_SparkFun" package="SO08" value="MOSFET-NCHANNEL-SOIC8"/>
<element name="MOTOR1" library="01_SparkFun" package="1X02_LONGPADS" value="DC"/>
<element name="C7" library="01_SparkFun" package="1206" value=".1 uf"/>
<element name="C8" library="01_SparkFun" package="1206" value="10 uf"/>
<element name="VCC_SERVO" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="PIN_SERVO" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="GND_SERVO" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="R1" library="01_FAB_Hello" package="1206" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="GND_SERVO" pad="1"/>
<contactref element="GND_SERVO" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="BATTERY" pad="2"/>
<contactref element="SV1" pad="2"/>
<contactref element="SV4" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="4"/>
<contactref element="U$3" pad="4"/>
<contactref element="VCC_SERVO" pad="2"/>
<contactref element="VCC_SERVO" pad="1"/>
<contactref element="SV1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SER2">
<contactref element="PIN_SERVO" pad="1"/>
<contactref element="SV4" pad="4"/>
</signal>
<signal name="SER1">
<contactref element="PIN_SERVO" pad="2"/>
<contactref element="SV4" pad="5"/>
</signal>
<signal name="OUT2">
<contactref element="MOTOR1" pad="1"/>
<contactref element="U$3" pad="8"/>
</signal>
<signal name="LSS">
<contactref element="U$1" pad="7"/>
<contactref element="U$3" pad="7"/>
</signal>
<signal name="OUT1">
<contactref element="MOTOR1" pad="2"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="VBB">
<contactref element="BATTERY" pad="1"/>
<contactref element="U$1" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="IN2">
<contactref element="U$3" pad="2"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="IN1">
<contactref element="U$3" pad="3"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="IN3">
<contactref element="U$1" pad="3"/>
<contactref element="SV4" pad="7"/>
</signal>
<signal name="IN4">
<contactref element="U$1" pad="2"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="OUT4">
<contactref element="MOTOR" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="OUT3">
<contactref element="MOTOR" pad="2"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="SV4" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
