<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0.8128" layer="20"/>
</plain>
<libraries>
<library name="fab2015">
<packages>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="fab2015" package="R1206FAB" value="1k"/>
<element name="U$2" library="fab2015" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$1" library="fab2015" package="2X02SMD" value="PINHD-2X2-SMD"/>
</elements>
<signals>
<signal name="R1">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
