ESP32-C3-Zero corrected KiCad files

Included files
- Waveshare_ESP32-C3-Zero_CASTELLATED.kicad_mod
- Waveshare_ESP32-C3-Zero.kicad_sym

Right side corrected order
Top -> bottom:
GPIO21, GPIO20, GPIO19, GPIO18, GPIO10, GPIO9, GPIO8, GPIO7, GPIO6

Pad mapping used in the symbol
Pad 10 = GPIO21
Pad 11 = GPIO20
Pad 12 = GPIO19
Pad 13 = GPIO18
Pad 14 = GPIO10
Pad 15 = GPIO9
Pad 16 = GPIO8
Pad 17 = GPIO7
Pad 18 = GPIO6

How to import footprint
1. Create a folder called Waveshare.pretty
2. Put Waveshare_ESP32-C3-Zero_CASTELLATED.kicad_mod inside it
3. In KiCad: Preferences > Manage Footprint Libraries
4. Add the folder Waveshare.pretty

How to import symbol
1. In KiCad Schematic Editor: Preferences > Manage Symbol Libraries
2. Add the file Waveshare_ESP32-C3-Zero.kicad_sym
3. Place symbol: ESP32-C3-Zero

Important
- The footprint is mechanical and approximate for the castellated breakout.
- Verify the real board with caliper before fabrication.
- Check the left-side pin order against your physical board before final production.
- Keep copper away from the antenna area.
