(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 2.33)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.4)
			)
			(layer "dielectric 1"
				(type "core")
				(color "#808080FF")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.4)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "/Users/christiannyqvist/Downloads/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(BUTTON_01-Pin_2)")
	(net 3 "Net-(BUTTON_02-Pin_2)")
	(net 4 "unconnected-(M1-3V3-Pad12)")
	(net 5 "5V+")
	(net 6 "D1{slash}A1")
	(net 7 "unconnected-(M1-GND-Pad13)")
	(net 8 "D3{slash}A3")
	(net 9 "D0{slash}A0")
	(net 10 "unconnected-(M1-SWCLK-Pad20)")
	(net 11 "unconnected-(M1-3V3-Pad12)_1")
	(net 12 "unconnected-(M1-D9-Pad10)")
	(net 13 "unconnected-(M1-D10-Pad11)")
	(net 14 "unconnected-(M1-D9-Pad10)_1")
	(net 15 "D4{slash}A4")
	(net 16 "unconnected-(M1-SWDIO-Pad17)")
	(net 17 "unconnected-(M1-RESET-Pad18)")
	(net 18 "D5{slash}A5")
	(net 19 "unconnected-(J1-Pin_4-Pad4)")
	(net 20 "unconnected-(M1-D10-Pad11)_1")
	(net 21 "unconnected-(M1-5V-Pad14)")
	(net 22 "unconnected-(M1-5V-Pad14)_1")
	(net 23 "unconnected-(M1-D6-Pad7)")
	(net 24 "unconnected-(M1-GND-Pad13)_1")
	(net 25 "unconnected-(J1-Pin_2-Pad2)")
	(net 26 "unconnected-(M1-D6-Pad7)_1")
	(net 27 "unconnected-(M1-GND-Pad19)")
	(net 28 "unconnected-(M1-D3-Pad4)")
	(net 29 "unconnected-(M1-D3-Pad4)_1")
	(net 30 "D9{slash}A9")
	(net 31 "unconnected-(M1-D2-Pad3)")
	(net 32 "unconnected-(M1-D2-Pad3)_1")
	(net 33 "Net-(PIR_SENSOR1-Pin_3)")
	(net 34 "unconnected-(J1-Pin_3-Pad3)")
	(net 35 "unconnected-(J1-Pin_1-Pad1)")
	(footprint "PCM_fab:Button_Omron_B3SN_6.0x6.0mm"
		(layer "F.Cu")
		(uuid "06093919-b352-43bf-9b6f-5c2d5c8080b1")
		(at 109.345 100.57)
		(descr "Surface Mount Tactile Switch for High-Density Packaging")
		(tags "Tactile Switch")
		(property "Reference" "TTEST_BUTTON_02"
			(at 0 -4 0)
			(layer "F.SilkS")
			(uuid "a807aad5-5c58-4696-a994-8b4e2b7e86cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Switch_Tactile_Omron"
			(at 0 4.5 0)
			(layer "F.Fab")
			(uuid "2d8b0f3e-2c63-40c0-b01f-c813b497b2af")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3sn.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d0ce2eb-67c6-45b9-a948-47284d5cabd0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, Omron, B3SN, Sealed Tactile Switch (SMT), SPST-NO Top Actuated Surface Mount"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc6d5701-83c7-4773-a71e-13aa6ae88536")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Button*")
		(path "/03e78589-e739-4af1-b886-a70c9c3d03ba")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.15 -3.15)
			(end 3.15 -3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf294838-5dd5-4065-a587-3da260d04a9b")
		)
		(fp_line
			(start -3.15 1)
			(end -3.15 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d152760b-9efe-4bd8-81d6-799114baa387")
		)
		(fp_line
			(start 3.15 -1)
			(end 3.15 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b119ca0-2816-4e58-87b3-f19ea5b75db2")
		)
		(fp_line
			(start 3.15 3.15)
			(end -3.15 3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd2b4cf8-101b-4c82-adff-1db9d0c2ed9e")
		)
		(fp_line
			(start -5 -3.7)
			(end -5 3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc5ed24c-a8fa-42df-b19b-ea7d6c9c70ad")
		)
		(fp_line
			(start -5 3.7)
			(end 5 3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f26d94c0-dee4-4e71-87ac-f7242bc105a2")
		)
		(fp_line
			(start 5 -3.7)
			(end -5 -3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd59aceb-53c1-452d-96a2-f9b0835d9bec")
		)
		(fp_line
			(start 5 3.7)
			(end 5 -3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c61762ce-837f-43fe-85f9-cae044568a28")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e17bc20-9e56-4e1d-a84b-e858beab05fc")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a15e0875-5372-4197-a9b4-4abc2b7d8642")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa9e7ed9-87b9-4f0b-86ef-78f4c3d8a38d")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b8cbb07-5f06-441e-a345-e58718a94865")
		)
		(fp_circle
			(center 0 0)
			(end 1.65 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7d57e08c-49bf-4d1a-82b7-02ddaa4a0140")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "eea80b49-6232-4082-b456-c680a720c9e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.5 -2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "D1{slash}A1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "b52349df-4775-4b47-b6bb-0e0752969233")
		)
		(pad "1" smd rect
			(at 3.5 -2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "D1{slash}A1")
			(pinfunction "1")
			(pintype "passive")
			(uuid "18a03e3b-72ed-47f9-a1c5-0747f7bba31c")
		)
		(pad "2" smd rect
			(at -3.5 2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(BUTTON_02-Pin_2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "832feb48-15ba-4093-995c-a3efa5300e4a")
		)
		(pad "2" smd rect
			(at 3.5 2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(BUTTON_02-Pin_2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "7c96a87a-83e4-4985-9d73-a4f933948b21")
		)
		(embedded_fonts no)
		(model "${KICAD9_3RD_PARTY}/3dmodels/org_fabcloud_gitlab_electronics_kicad/fab.3dshapes/Switch_Omron-B3SN-3112P.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "PCM_fab:TerminalBlock_OnShore_1x02_P5.00mm_Horizontal"
		(layer "F.Cu")
		(uuid "28069452-948e-41ae-bea4-e373d3a59435")
		(at 87.845 89.97)
		(descr "2 Position Wire to Board Terminal Block Horizontal with Board 0.197\" (5.00mm) Through Hole")
		(tags "THT Terminal Block pitch 5mm")
		(property "Reference" "BUTTON_01"
			(at 2.5 -5 0)
			(layer "F.SilkS")
			(uuid "6beae362-f636-4e71-8a0d-159e8b293f99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x02_P5mm"
			(at 2.5 6.3 0)
			(layer "F.Fab")
			(uuid "2e0bdc3d-54ae-4bbc-b1ae-68e3d6927bb3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.on-shore.com/wp-content/uploads/OSTTAXX0161.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "34b3001a-d246-40e2-8edf-dc5b4f5cad0e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "TERM BLK 2POS SIDE ENTRY 5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0267e6fe-b543-4ffb-87e2-7d265323a32b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*TerminalBlock*1x02*P5.00mm*")
		(path "/0254933d-10cc-43b7-a908-f163c93e6d66")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -3.1 -4)
			(end -3.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13a03697-06ad-41dd-aca4-762fdda40140")
		)
		(fp_line
			(start -3.1 -4)
			(end 8.1 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "588d988c-987b-4ce2-ac2f-f47bcfc0b15d")
		)
		(fp_line
			(start -3.1 5.2)
			(end 8.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c6bd8b3-bab6-4d89-a34a-7d6d378964ea")
		)
		(fp_line
			(start 8.1 -4)
			(end 8.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ebfe9b1c-7fa9-4537-8319-cc362e8b84f8")
		)
		(fp_line
			(start -3 -3.9)
			(end -3 5.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d1e9096-4186-4d7f-ba78-f7fafe064a2a")
		)
		(fp_line
			(start -3 5.1)
			(end 8 5.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "915844e4-0902-4bb1-ba7f-20eeaae7fbc1")
		)
		(fp_line
			(start 8 -3.9)
			(end -3 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c9bb162-dd88-4400-b922-fbc78a16803d")
		)
		(fp_line
			(start 8 5.1)
			(end 8 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "653bdeaf-af46-473a-8bc1-b6815a37123d")
		)
		(fp_line
			(start -3 -3.9)
			(end 8 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc9fc558-853f-46ca-9b32-1f94b0454863")
		)
		(fp_line
			(start -3 4.5)
			(end -3 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30e2bf5b-c5e6-45dc-9510-caf9cf76090d")
		)
		(fp_line
			(start -2.4 5.1)
			(end -3 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f807ed48-debc-4fd1-99ec-d13301fa6d6e")
		)
		(fp_line
			(start 8 -3.9)
			(end 8 5.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83d9ba34-4db4-4a75-ad68-2203d62b4456")
		)
		(fp_line
			(start 8 5.1)
			(end -2.4 5.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2984fc64-a031-4471-850d-cb88c3d8c6e7")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.8 0)
			(layer "F.Fab")
			(uuid "28773660-7986-4efc-975a-c72aed547e39")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e5aec746-2dd6-4de1-bcad-fe6e6a3446eb")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(BUTTON_01-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "975c9e88-7b61-44ec-b147-f8e59d1f296a")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_fab:Button_Omron_B3SN_6.0x6.0mm"
		(layer "F.Cu")
		(uuid "2ddb56c1-9ff6-440e-a5f9-793e6c8b006f")
		(at 109.345 88.57)
		(descr "Surface Mount Tactile Switch for High-Density Packaging")
		(tags "Tactile Switch")
		(property "Reference" "TEST_BUTTON_01"
			(at 0 -4 0)
			(layer "F.SilkS")
			(uuid "942766a5-6430-4088-873b-86f66826e0c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Switch_Tactile_Omron"
			(at 0 4.5 0)
			(layer "F.Fab")
			(uuid "1116a442-1de6-4322-8c92-66f8428ebb14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3sn.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d468247d-5d00-419f-8cfd-59e7716b1b8f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, Omron, B3SN, Sealed Tactile Switch (SMT), SPST-NO Top Actuated Surface Mount"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac91a968-ed45-41c8-94d0-52f02400dfbd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Button*")
		(path "/2e0f23e4-42a4-412b-b0e1-7e4e2dc7f88e")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.15 -3.15)
			(end 3.15 -3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dff1ba39-9004-46d5-bbe5-2a0e4327d811")
		)
		(fp_line
			(start -3.15 1)
			(end -3.15 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fcb931f-fd3b-4764-8685-3cd9a6438c7e")
		)
		(fp_line
			(start 3.15 -1)
			(end 3.15 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ece68663-267f-4b60-849d-29121839bf91")
		)
		(fp_line
			(start 3.15 3.15)
			(end -3.15 3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7debad79-0c58-40c1-ae59-60a120e9f429")
		)
		(fp_line
			(start -5 -3.7)
			(end -5 3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40284785-d44b-4b66-94e0-c727db1dbabf")
		)
		(fp_line
			(start -5 3.7)
			(end 5 3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c1740f48-e5f1-42d9-8dbb-5ca7067afc59")
		)
		(fp_line
			(start 5 -3.7)
			(end -5 -3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "56b75a0a-b1dd-4cbc-be3a-b7cbf7e2eec3")
		)
		(fp_line
			(start 5 3.7)
			(end 5 -3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cada7101-ff79-4c4e-ad02-2c412163950d")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df7a9e73-2e26-481d-bd4c-1ada2d9b40ac")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7fdcd41b-25b7-4582-8c53-ff391816f1c4")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95fa2ace-38f0-4293-8387-dab76cd17432")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1688b9af-6c91-4d6f-8f98-214db2918f9d")
		)
		(fp_circle
			(center 0 0)
			(end 1.65 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "1b44c6ce-adb9-4222-9261-d59145c15b00")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "0ffc36b0-5c62-44fd-b507-7833f313c2ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.5 -2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "D0{slash}A0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "4bd4e11c-2533-430f-a9bd-8f12123be1a7")
		)
		(pad "1" smd rect
			(at 3.5 -2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "D0{slash}A0")
			(pinfunction "1")
			(pintype "passive")
			(uuid "cf9e867d-edf5-42ff-bba9-10e372ef6130")
		)
		(pad "2" smd rect
			(at -3.5 2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(BUTTON_01-Pin_2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "a6b291dd-adc1-4efe-a1f5-426ea912146f")
		)
		(pad "2" smd rect
			(at 3.5 2)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(BUTTON_01-Pin_2)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "aaefddec-a302-4af7-84bb-7aa75a724779")
		)
		(embedded_fonts no)
		(model "${KICAD9_3RD_PARTY}/3dmodels/org_fabcloud_gitlab_electronics_kicad/fab.3dshapes/Switch_Omron-B3SN-3112P.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "PCM_fab:TerminalBlock_OnShore_1x02_P5.00mm_Horizontal"
		(layer "F.Cu")
		(uuid "3e3b3193-d8e2-455a-a1d2-b10730d88600")
		(at 106.5 114.5)
		(descr "2 Position Wire to Board Terminal Block Horizontal with Board 0.197\" (5.00mm) Through Hole")
		(tags "THT Terminal Block pitch 5mm")
		(property "Reference" "POWER_INPUT1"
			(at 2.5 -5 0)
			(layer "F.SilkS")
			(uuid "fcb959b3-faad-42e5-a821-e68a01789d5e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x02_P5mm"
			(at 2.5 6.3 0)
			(layer "F.Fab")
			(uuid "f11f3ec8-7884-4e9e-b651-3e5b3de2b685")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.on-shore.com/wp-content/uploads/OSTTAXX0161.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "73dc66f4-11a8-43fb-8658-8491874c366e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "TERM BLK 2POS SIDE ENTRY 5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1631d050-ff2c-46db-ba7d-3ec74f395f3d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*TerminalBlock*1x02*P5.00mm*")
		(path "/13e61221-91af-4fec-b068-426345e6b5e2")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -3.1 -4)
			(end -3.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f716ea4-282d-48b4-97b5-737b3ffc84f4")
		)
		(fp_line
			(start -3.1 -4)
			(end 8.1 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc8a8bc8-b73f-4444-9e02-927f40758783")
		)
		(fp_line
			(start -3.1 5.2)
			(end 8.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de93fcdc-9459-4c03-a7f6-02bad272b45a")
		)
		(fp_line
			(start 8.1 -4)
			(end 8.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d7d3cd6-e212-4776-8464-7e25b47a6741")
		)
		(fp_line
			(start -3 -3.9)
			(end -3 5.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e976b47f-06b2-451e-a473-f79e6065867a")
		)
		(fp_line
			(start -3 5.1)
			(end 8 5.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47ab423f-1459-4a3d-bbfe-dfe8c02a0fe7")
		)
		(fp_line
			(start 8 -3.9)
			(end -3 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d691c656-be32-4fbf-aeaa-b4e49ffd49d7")
		)
		(fp_line
			(start 8 5.1)
			(end 8 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6ef495cb-7c6b-4f79-97a2-a681b1787fac")
		)
		(fp_line
			(start -3 -3.9)
			(end 8 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d65d6e07-5776-4a5f-be6f-aa6620ba4a91")
		)
		(fp_line
			(start -3 4.5)
			(end -3 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a4780e7-a396-4a82-88ac-a66a4ac18efa")
		)
		(fp_line
			(start -2.4 5.1)
			(end -3 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1270e14f-306c-4518-b704-d2e95a7515c6")
		)
		(fp_line
			(start 8 -3.9)
			(end 8 5.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d08276f-1e27-4e3f-be36-f4e8d64654e2")
		)
		(fp_line
			(start 8 5.1)
			(end -2.4 5.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc507015-443c-48f2-b508-3ec95a1ac549")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.8 0)
			(layer "F.Fab")
			(uuid "45bd2115-6e17-48c8-8522-3450ca009ad8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "006e8b24-d411-457b-b939-c457143b8fa8")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "5V+")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "8c13d4cd-2392-4cca-bd78-9c7fac9e7042")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_fab:Button_Omron_B3SN_6.0x6.0mm"
		(layer "F.Cu")
		(uuid "58643d2b-cc5d-42eb-95eb-a2bb27608937")
		(at 163 103.5 -90)
		(descr "Surface Mount Tactile Switch for High-Density Packaging")
		(tags "Tactile Switch")
		(property "Reference" "TEST_BUTTON_PIR_SENSOR1"
			(at 0 -4 90)
			(layer "F.SilkS")
			(uuid "787ef7ce-7f0f-423f-a7be-3de1cd8bc2be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Switch_Tactile_Omron"
			(at 0 4.5 90)
			(layer "F.Fab")
			(uuid "b5fc6ef3-9577-4b01-8f9a-fcd9f80b80b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3sn.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5abc6cf3-8ba6-4fd5-946f-e7dde2674f94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Push button switch, Omron, B3SN, Sealed Tactile Switch (SMT), SPST-NO Top Actuated Surface Mount"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6220007-39dd-4df7-a573-9393373efa1b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*Button*")
		(path "/ddeafd57-b358-47bd-bf3b-e377b2ba302f")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr smd)
		(fp_line
			(start 3.15 3.15)
			(end -3.15 3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1faa1f6e-c40f-4094-8318-58b57fa6f89b")
		)
		(fp_line
			(start -3.15 1)
			(end -3.15 -1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b438c8c7-1f80-4713-b311-47272752ed5f")
		)
		(fp_line
			(start 3.15 -1)
			(end 3.15 1)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6b4c0b2-c0b7-43e4-8b9c-e546279831de")
		)
		(fp_line
			(start -3.15 -3.15)
			(end 3.15 -3.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "545b5b37-cc67-4a4f-b536-de15e685c876")
		)
		(fp_line
			(start -5 3.7)
			(end 5 3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "774cf6cc-b336-4951-8213-ff1b31c2f9d6")
		)
		(fp_line
			(start 5 3.7)
			(end 5 -3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "deda5d85-3e3a-4426-aafc-c52df9705b79")
		)
		(fp_line
			(start -5 -3.7)
			(end -5 3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "291233bd-9726-4277-bd8e-cf2c6f59f3df")
		)
		(fp_line
			(start 5 -3.7)
			(end -5 -3.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "69303e12-4981-43d4-bbc1-9fa6ec0b532e")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "664bb513-4c08-411d-b73c-0aed8429a6ff")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96f3d214-1c1a-476c-9ae8-34135ee2c9f9")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43a9aa81-e9dc-4b00-b0fd-168b6f965ed1")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "985f4e76-f5c1-4b12-9495-c1f1650e17d5")
		)
		(fp_circle
			(center 0 0)
			(end 1.65 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5a0f6488-cb9f-4081-a551-be9a0d7fc5d6")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "19d83b22-84d7-432b-8a28-a63968845038")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -3.5 -2 270)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(PIR_SENSOR1-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "69aae2cb-1346-48fe-87c1-ceefe83d7f1b")
		)
		(pad "1" smd rect
			(at 3.5 -2 270)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(PIR_SENSOR1-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "3ca25f7c-5562-426c-b16a-f86f23ea717f")
		)
		(pad "2" smd rect
			(at -3.5 2 270)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "D9{slash}A9")
			(pinfunction "2")
			(pintype "passive")
			(uuid "4384d10f-78fe-43b1-8313-a8e4b65f6b43")
		)
		(pad "2" smd rect
			(at 3.5 2 270)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "D9{slash}A9")
			(pinfunction "2")
			(pintype "passive")
			(uuid "bf52536e-ae1d-4fc7-b4ca-1dd990c5fdd5")
		)
		(embedded_fonts no)
		(model "${KICAD9_3RD_PARTY}/3dmodels/org_fabcloud_gitlab_electronics_kicad/fab.3dshapes/Switch_Omron-B3SN-3112P.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "PCM_fab:TerminalBlock_OnShore_1x03_P3.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "8310858e-aa0d-48a7-b3e0-9a37f2e68692")
		(at 144 117.05 180)
		(descr "3 Position Wire to Board Terminal Block Horizontal with Board 0.138\" (3.50mm) Through Hole")
		(tags "THT Terminal Block pitch 3.5mm")
		(property "Reference" "RELAY_PINS1"
			(at 3.8 -3.9 0)
			(layer "F.SilkS")
			(uuid "2d3b258b-6181-49f3-a167-2f19eece1e7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03_P3.5mm"
			(at 4.2 5.5 0)
			(layer "F.Fab")
			(uuid "3012052a-4be7-4cea-8f56-47c8e3f281ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "www.on-shore.com/wp-content/uploads/ED555XDS.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "749eb037-4f80-4c71-83b3-80644670c297")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "TERM BLK 3POS SIDE ENT 3.5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b211d14c-f389-4612-9c74-59d0f12439f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*TerminalBlock*1x03*P3.50mm*")
		(path "/11dee806-b1fa-48e6-97be-98c0baaee320")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 8.9 -2.8)
			(end 8.9 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23e92834-2c75-46ed-87df-affb9cf40047")
		)
		(fp_line
			(start -1.9 3.9)
			(end 8.9 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0d20e67-634f-42ae-bba3-e8cf2eb8010f")
		)
		(fp_line
			(start -1.9 -2.8)
			(end 8.9 -2.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4bc76da6-5403-4989-bf38-5243d12f622f")
		)
		(fp_line
			(start -1.9 -2.8)
			(end -1.9 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6e4ed0b-2392-4d77-b63e-d0ff86f1e7d5")
		)
		(fp_line
			(start 8.8 3.8)
			(end 8.8 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6833dc05-4ff2-4317-af99-e08590a22608")
		)
		(fp_line
			(start 8.8 -2.7)
			(end -1.8 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5293f39e-0da5-4929-a88a-d2883c55a57c")
		)
		(fp_line
			(start -1.8 3.8)
			(end 8.8 3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4022f7c6-97b6-4ebc-a373-8521916c6ada")
		)
		(fp_line
			(start -1.8 -2.7)
			(end -1.8 3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce697f18-5b47-4764-9a97-d4a3d5fa8551")
		)
		(fp_line
			(start 8.8 3.8)
			(end -0.7 3.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9a60d0a-8621-4fc9-803d-fe3bfa1b5c55")
		)
		(fp_line
			(start 8.8 -2.7)
			(end 8.8 3.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00c391ae-9ac2-4679-9b01-683260ca4724")
		)
		(fp_line
			(start -0.7 3.8)
			(end -1.8 2.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07c7436d-969d-4f95-9d18-8c6c5cd8776f")
		)
		(fp_line
			(start -1.8 2.7)
			(end -1.8 -2.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7fece54-936a-4bd5-afa4-1e4b16692825")
		)
		(fp_line
			(start -1.8 -2.7)
			(end 8.8 -2.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00ed5a89-9a6a-43fb-8201-59de704dcf4a")
		)
		(fp_text user "${REFERENCE}"
			(at 4 2.9 0)
			(layer "F.Fab")
			(uuid "1bce7fa5-8922-4e83-b4ee-03fb40558016")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D3{slash}A3")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "ca8fe22b-e3d2-4fa5-abc7-78f4414a31e9")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ec0aea33-c8b7-4d32-8369-fd0807e8f958")
		)
		(pad "3" thru_hole circle
			(at 7 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "5V+")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "24c8e18d-341f-4a45-b2e6-d645b4977d61")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_fab:SeeedStudio_XIAO_RP2040"
		(layer "F.Cu")
		(uuid "8bd6de3c-291e-4826-ab0d-8264ad5a264d")
		(at 138.725 94.11)
		(descr "Footprint for Seeed Studio XIAO modules")
		(tags "xiao seeed studio module")
		(property "Reference" "M1"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "52d0bb7e-58bf-4278-bc08-25de9d2e2856")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Module_XIAO-RP2040"
			(at 0.005 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "da645c05-e78c-40e5-970a-4494e0c22a07")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2928766a-22ec-41c2-b413-a8c74a69906a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Dual-Core Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b38bcedf-fb4d-4ad1-a1af-2057680b4eee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?RP2040*")
		(path "/77d69373-5a82-4802-a4a1-f6ebb963c415")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -8.8875 9.281)
			(end -8.8875 -9.261)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f2802b6-ba8a-42bb-80ce-f6797490466f")
		)
		(fp_line
			(start -7.6175 -10.531)
			(end 7.6225 -10.531)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52bf4da8-dbe8-442c-b78a-e003fd641e11")
		)
		(fp_line
			(start 7.6225 10.551)
			(end -7.6175 10.551)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e84e38b-55e9-4014-a1d2-4ff9b44674bc")
		)
		(fp_line
			(start 8.8925 -9.261)
			(end 8.8925 9.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a300e056-6a5c-4ec6-a811-64c98e724265")
		)
		(fp_rect
			(start -4.4975 -10.531)
			(end 4.5025 -12.055)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "57ce7673-7b08-4d58-b600-5bb80ff42044")
		)
		(fp_arc
			(start -8.8875 -9.261)
			(mid -8.515526 -10.159026)
			(end -7.6175 -10.531)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "888dae1b-ac21-4c96-8947-166e0ee5a856")
		)
		(fp_arc
			(start -7.6175 10.551)
			(mid -8.515526 10.179026)
			(end -8.8875 9.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e9f1bc2-114b-4fd5-b01b-4d5b41438fc7")
		)
		(fp_arc
			(start 7.6225 -10.531)
			(mid 8.520526 -10.159026)
			(end 8.8925 -9.261)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b167a0fa-0798-43eb-84f0-6e98ca322554")
		)
		(fp_arc
			(start 8.8925 9.281)
			(mid 8.520526 10.179026)
			(end 7.6225 10.551)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4f28502-86c4-4bb6-8a94-ad4b82ae5d99")
		)
		(fp_rect
			(start -10.315 -12.38)
			(end 10.285 10.82)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "d93611e1-68a8-467f-9181-d7516eb302e8")
		)
		(fp_text user "VIN"
			(at -2.535 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "0720abc9-140f-4bef-a8c7-2066d82e8dbd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "GND"
			(at 2.545 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "439fab96-bffd-4c7b-b9e8-78a1d545adef")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "GND"
			(at 2.54 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "49d3a3b8-0d28-482c-9773-46daa1257bba")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "RESET"
			(at 0 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "5a6843be-e869-4533-80b1-cfc88300d673")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "SWCLK"
			(at 2.54 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "8bb66c21-3e2f-4667-8625-7ebe25f6a6c2")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "SWDIO"
			(at 0 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "f909ea70-3b42-47c1-8720-75c9c87aabbf")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.1)
					(bold yes)
				)
			)
		)
		(fp_text user "${REFERENCE}"
			(at 0.0025 3.81 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "6ec5858f-e6e8-42fb-aa0c-65177ead816f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at -7.615 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D0{slash}A0")
			(pinfunction "D0")
			(pintype "bidirectional")
			(uuid "a5d1e989-9d6c-4154-b3ad-79a0a420face")
		)
		(pad "1" smd rect
			(at -7.615 -7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "D0{slash}A0")
			(pinfunction "D0")
			(pintype "bidirectional")
			(uuid "1719bf52-c5e1-4554-953f-3963955bfff0")
		)
		(pad "2" thru_hole circle
			(at -7.615 -5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "D1{slash}A1")
			(pinfunction "D1")
			(pintype "bidirectional")
			(uuid "ba1a6e17-c3ee-45a6-a6ec-a50e352639ab")
		)
		(pad "2" smd rect
			(at -7.615 -5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "D1{slash}A1")
			(pinfunction "D1")
			(pintype "bidirectional")
			(uuid "7f52ff7a-378c-4e55-96dd-73559c1a0f5c")
		)
		(pad "3" thru_hole circle
			(at -7.615 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(M1-D2-Pad3)_1")
			(pinfunction "D2")
			(pintype "bidirectional+no_connect")
			(uuid "ef7cfe96-ad96-41ff-999a-bac7b7cc02d0")
		)
		(pad "3" smd rect
			(at -7.615 -2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(M1-D2-Pad3)")
			(pinfunction "D2")
			(pintype "bidirectional+no_connect")
			(uuid "4688f43e-5cdf-4220-9cce-2dc73f8856d4")
		)
		(pad "4" thru_hole circle
			(at -7.615 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(M1-D3-Pad4)_1")
			(pinfunction "D3")
			(pintype "bidirectional+no_connect")
			(uuid "b80a8deb-5d9c-4baf-91a8-2cffe09f8194")
		)
		(pad "4" smd rect
			(at -7.615 0)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(M1-D3-Pad4)")
			(pinfunction "D3")
			(pintype "bidirectional+no_connect")
			(uuid "27dd2501-dee7-47cc-b9e2-5439b7f08e01")
		)
		(pad "5" thru_hole circle
			(at -7.615 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D4{slash}A4")
			(pinfunction "D4")
			(pintype "bidirectional")
			(uuid "7b1fc484-0d62-4d0f-ad15-9eed31915b38")
		)
		(pad "5" smd rect
			(at -7.615 2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "D4{slash}A4")
			(pinfunction "D4")
			(pintype "bidirectional")
			(uuid "c5eae7ee-9df9-4fdb-bb2c-b3358e057096")
		)
		(pad "6" thru_hole circle
			(at -7.615 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "D5{slash}A5")
			(pinfunction "D5")
			(pintype "bidirectional")
			(uuid "2ef84534-f3d9-4b0d-9f52-ad70bdf9a593")
		)
		(pad "6" smd rect
			(at -7.615 5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "D5{slash}A5")
			(pinfunction "D5")
			(pintype "bidirectional")
			(uuid "70e72288-ff7c-4c92-8d57-23c02091a300")
		)
		(pad "7" thru_hole circle
			(at -7.615 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(M1-D6-Pad7)")
			(pinfunction "D6")
			(pintype "bidirectional+no_connect")
			(uuid "0eaf73e0-0a0c-44a1-91a7-6a15f30994d3")
		)
		(pad "7" smd rect
			(at -7.615 7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(M1-D6-Pad7)_1")
			(pinfunction "D6")
			(pintype "bidirectional+no_connect")
			(uuid "ba88653e-7a04-4453-b364-1f65602bd853")
		)
		(pad "8" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D3{slash}A3")
			(pinfunction "D7")
			(pintype "bidirectional")
			(uuid "8c6fbcb5-4ff3-4926-ba03-d44dc9eca230")
		)
		(pad "8" smd rect
			(at 7.62 7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "D3{slash}A3")
			(pinfunction "D7")
			(pintype "bidirectional")
			(uuid "06cd3d1a-3e70-468f-9e9a-d6eec19d2224")
		)
		(pad "9" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "D9{slash}A9")
			(pinfunction "D8")
			(pintype "bidirectional")
			(uuid "09b0bbef-f697-4d8f-8441-f7741f4461a4")
		)
		(pad "9" smd rect
			(at 7.62 5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "D9{slash}A9")
			(pinfunction "D8")
			(pintype "bidirectional")
			(uuid "b64f0da3-1467-421a-a733-5e1b6dbcffb6")
		)
		(pad "10" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(M1-D9-Pad10)")
			(pinfunction "D9")
			(pintype "bidirectional+no_connect")
			(uuid "0988ed16-693c-408b-afca-25ef4d106b83")
		)
		(pad "10" smd rect
			(at 7.62 2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(M1-D9-Pad10)_1")
			(pinfunction "D9")
			(pintype "bidirectional+no_connect")
			(uuid "b8111ddd-a28b-418c-97bf-52086b360787")
		)
		(pad "11" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(M1-D10-Pad11)")
			(pinfunction "D10")
			(pintype "bidirectional+no_connect")
			(uuid "3a5c3695-c4b5-433b-83ac-96ec9c58df06")
		)
		(pad "11" smd rect
			(at 7.62 0)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(M1-D10-Pad11)_1")
			(pinfunction "D10")
			(pintype "bidirectional+no_connect")
			(uuid "b26c8837-c4eb-4615-bcfd-e20361765b1b")
		)
		(pad "12" thru_hole circle
			(at 7.62 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(M1-3V3-Pad12)_1")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
			(uuid "facad4cb-2152-4584-99a3-3797e3a2d487")
		)
		(pad "12" smd rect
			(at 7.62 -2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(M1-3V3-Pad12)")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
			(uuid "8300b426-1204-4588-995c-9bec5b1f2cec")
		)
		(pad "13" thru_hole circle
			(at 7.62 -5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(M1-GND-Pad13)_1")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
			(uuid "d77c3fe5-d008-4138-9f43-72caaa192b4c")
		)
		(pad "13" smd rect
			(at 7.62 -5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(M1-GND-Pad13)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
			(uuid "77235aaa-9161-44fb-8109-82c05ed81838")
		)
		(pad "14" thru_hole circle
			(at 7.62 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(M1-5V-Pad14)")
			(pinfunction "5V")
			(pintype "power_in+no_connect")
			(uuid "6ee70c61-5837-4538-bc75-7883522b4a40")
		)
		(pad "14" smd rect
			(at 7.62 -7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(M1-5V-Pad14)_1")
			(pinfunction "5V")
			(pintype "power_in+no_connect")
			(uuid "e3bac739-38ae-4e63-b0f0-7e67faaf0b21")
		)
		(pad "15" smd rect
			(at 1.275 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "ab447f01-0826-4d7d-b523-e095b52d48c7")
		)
		(pad "16" smd rect
			(at -1.265 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "5V+")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "012b9f51-ee54-423e-b06e-1d1bc0e84ec5")
		)
		(pad "17" smd circle
			(at -1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(M1-SWDIO-Pad17)")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
			(uuid "e354d748-529b-4ae6-9d82-8ebd0a3972cf")
		)
		(pad "18" smd circle
			(at -1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(M1-RESET-Pad18)")
			(pinfunction "RESET")
			(pintype "input+no_connect")
			(uuid "0f5fb71d-5bd7-45f9-9be1-2f89e9ca4448")
		)
		(pad "19" smd circle
			(at 1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(M1-GND-Pad19)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
			(uuid "22dc5516-4c2d-471b-a4fd-8c64d0c97978")
		)
		(pad "20" smd circle
			(at 1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(M1-SWCLK-Pad20)")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
			(uuid "736e4b71-9623-42d8-b764-b1f22e837a7c")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(uuid "a3946146-1ec9-4dce-97e7-c263f7e3bcf0")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 133.525 83.56) (xy 134.925 83.56) (xy 134.925 85.61) (xy 133.525 85.61)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(uuid "89ff5256-ebc5-4267-a100-22ed09840da2")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 133.525 87.61) (xy 134.925 87.61) (xy 134.925 89.81) (xy 133.525 89.81)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(uuid "29b80b4d-dc47-402b-8a22-937ece91bc07")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 142.525 83.56) (xy 143.925 83.56) (xy 143.925 85.61) (xy 142.525 85.61)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(uuid "58940fe7-6f4b-49d0-9de0-8a9a11333771")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 142.525 87.61) (xy 143.925 87.61) (xy 143.925 89.81) (xy 142.525 89.81)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3RD_PARTY}/3dmodels/org_fabcloud_gitlab_electronics_kicad/fab.3dshapes/Seeed_XIAO-nRF52840_Sense.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
	)
	(footprint "PCM_fab:TerminalBlock_OnShore_1x02_P5.00mm_Horizontal"
		(layer "F.Cu")
		(uuid "b3fcf357-aa06-4211-9594-65a1bed90bbf")
		(at 87.675 104.52)
		(descr "2 Position Wire to Board Terminal Block Horizontal with Board 0.197\" (5.00mm) Through Hole")
		(tags "THT Terminal Block pitch 5mm")
		(property "Reference" "BUTTON_02"
			(at 2.5 -5 0)
			(layer "F.SilkS")
			(uuid "ec359a04-bed1-4d05-9a54-4b2c6374e649")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x02_P5mm"
			(at 2.5 6.3 0)
			(layer "F.Fab")
			(uuid "fe64f691-c9c3-4225-85ef-4f9c542d4846")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.on-shore.com/wp-content/uploads/OSTTAXX0161.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "68c515b5-990f-47d2-9a0b-3936d6d52b2f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "TERM BLK 2POS SIDE ENTRY 5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2eefa854-543b-4d75-9b04-1cfd6dcfa795")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*TerminalBlock*1x02*P5.00mm*")
		(path "/b0bab118-4e45-472f-a824-0b762b5538a0")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -3.1 -4)
			(end -3.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ece5eb5-8b4d-49e0-8aa5-e4acc749e2c3")
		)
		(fp_line
			(start -3.1 -4)
			(end 8.1 -4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e72ce11-0572-4335-adec-6c5568aa4f5b")
		)
		(fp_line
			(start -3.1 5.2)
			(end 8.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae6c03d2-c56b-4dbb-825d-327800f3ee9e")
		)
		(fp_line
			(start 8.1 -4)
			(end 8.1 5.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3dd48d8-0883-4c12-acf6-2890b33ce983")
		)
		(fp_line
			(start -3 -3.9)
			(end -3 5.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4588f67-095e-4189-bf7a-a5f9198f7b3d")
		)
		(fp_line
			(start -3 5.1)
			(end 8 5.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f7f6ccc-4270-4f56-bf3a-b823bc245884")
		)
		(fp_line
			(start 8 -3.9)
			(end -3 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "01da23f7-a4b0-461a-9519-01c95dcb0ead")
		)
		(fp_line
			(start 8 5.1)
			(end 8 -3.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3659e5b-1489-446d-9181-1607ddaa90d0")
		)
		(fp_line
			(start -3 -3.9)
			(end 8 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cab0093-9fac-45aa-b488-296867039d99")
		)
		(fp_line
			(start -3 4.5)
			(end -3 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3cc00f6c-94ea-4622-a3e5-231b29f89f9c")
		)
		(fp_line
			(start -2.4 5.1)
			(end -3 4.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "92188c08-e83b-4168-a5f3-fd2be65348e3")
		)
		(fp_line
			(start 8 -3.9)
			(end 8 5.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84325596-81e8-4a44-bdfd-caee9daba84c")
		)
		(fp_line
			(start 8 5.1)
			(end -2.4 5.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5cc1c1ab-0e09-4cc7-8b82-6deedd05b365")
		)
		(fp_text user "${REFERENCE}"
			(at 2.5 2.8 0)
			(layer "F.Fab")
			(uuid "c6d92c83-788b-4faf-9396-da100482050f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "514b436c-a19f-46b6-97ef-b030f4bf510a")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(BUTTON_02-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "c3e4dcf6-95ba-4466-8db5-a6a737ae99d7")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_Philmore.3dshapes/TerminalBlock_Philmore_TB132_1x02_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_fab:TerminalBlock_OnShore_1x03_P3.50mm_Horizontal"
		(layer "F.Cu")
		(uuid "cba3da19-c444-424b-b9c3-f9746b94f638")
		(at 158.5 86.5)
		(descr "3 Position Wire to Board Terminal Block Horizontal with Board 0.138\" (3.50mm) Through Hole")
		(tags "THT Terminal Block pitch 3.5mm")
		(property "Reference" "PIR_SENSOR1"
			(at 3.8 -3.9 0)
			(layer "F.SilkS")
			(uuid "5a15f5f5-df7d-40c7-a306-a188f0136ae2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03_P3.5mm"
			(at 4.2 5.5 0)
			(layer "F.Fab")
			(uuid "477ed047-df21-45a4-8bf8-9b8f4f0cfa0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "www.on-shore.com/wp-content/uploads/ED555XDS.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8df62c6-db6a-48a0-b49a-a1ffc96851ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "TERM BLK 3POS SIDE ENT 3.5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "db64ced0-55e4-4144-ada2-11dbdff2c4e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*TerminalBlock*1x03*P3.50mm*")
		(path "/2f219f53-6c74-4435-af53-a8d6eb3f37ba")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -1.9 -2.8)
			(end -1.9 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3902eb7-3fe6-4eaf-b7b4-37b62ad30f81")
		)
		(fp_line
			(start -1.9 -2.8)
			(end 8.9 -2.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a41812b1-6875-4dd4-82a5-70a421fc1283")
		)
		(fp_line
			(start -1.9 3.9)
			(end 8.9 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14447031-acf7-437c-bbf4-a0f10f80222f")
		)
		(fp_line
			(start 8.9 -2.8)
			(end 8.9 3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "266a21a6-a921-47cb-a652-d1405278dfca")
		)
		(fp_line
			(start -1.8 -2.7)
			(end -1.8 3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d70a2ff-2df1-4046-a856-0ed2d9a6496d")
		)
		(fp_line
			(start -1.8 3.8)
			(end 8.8 3.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "caed5656-222a-4b56-9ebb-762547ae87ae")
		)
		(fp_line
			(start 8.8 -2.7)
			(end -1.8 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "680f66ba-a399-42f3-b139-cb10e39ed9ca")
		)
		(fp_line
			(start 8.8 3.8)
			(end 8.8 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab7cc1ee-45f1-4127-8240-8a1fb7b3607a")
		)
		(fp_line
			(start -1.8 -2.7)
			(end 8.8 -2.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42f5c25b-cf5c-4083-82af-952d280a0540")
		)
		(fp_line
			(start -1.8 2.7)
			(end -1.8 -2.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4cd43695-e374-4fcc-9639-47b58ccc8b5b")
		)
		(fp_line
			(start -0.7 3.8)
			(end -1.8 2.7)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6753818-4e97-4a28-8c60-d1b2475a3000")
		)
		(fp_line
			(start 8.8 -2.7)
			(end 8.8 3.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6974b0f9-5530-4a0c-a711-4237584cdf99")
		)
		(fp_line
			(start 8.8 3.8)
			(end -0.7 3.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "adbf9ac0-8747-4e6c-ab60-092dc61010bd")
		)
		(fp_text user "${REFERENCE}"
			(at 4 2.5 0)
			(layer "F.Fab")
			(uuid "4c64e85c-0df5-4979-be06-6da4a282cb54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "5V+")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "318df1bd-168b-4d1b-a465-27492cdee3e4")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "f7729cf8-64b7-40d1-903c-c3b7fde356da")
		)
		(pad "3" thru_hole circle
			(at 7 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(PIR_SENSOR1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "ffebd8ce-4946-45a9-89c6-3f1af6e9e7d0")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_fab:PinHeader_02x04_P2.54mm_Vertical_SMD"
		(layer "F.Cu")
		(uuid "ee086164-10a2-42cd-942f-e70364892d38")
		(at 121.5 107.5 180)
		(descr "surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x04 2.54mm double row")
		(property "Reference" "J1"
			(at 0 -6.14 0)
			(layer "F.SilkS")
			(uuid "4b8a2da1-b888-41cd-8611-5bd101d82ec8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "PinHeader_02x04_P2.54mm_Vertical_SMD"
			(at 0 6.14 0)
			(layer "F.Fab")
			(uuid "eee0cbf6-4e7d-4058-9796-d737fd53b494")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e020aa21-dc5c-44c2-a36f-de7bc6588779")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Connector Header Surface Mount 8 position 0.100\" (2.54mm)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7568ee11-3e44-4317-80da-ebfdffeca350")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "*PinHeader*2x04*")
		(path "/43eaffd8-58bd-470a-ac4a-c40514f714bd")
		(sheetname "/")
		(sheetfile "LetThereBeLight_I2C.kicad_sch")
		(attr smd)
		(fp_line
			(start 2.6 4.57)
			(end 2.6 5.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94280fd4-365b-4ed5-8220-8cddeb76eef5")
		)
		(fp_line
			(start 2.6 2.03)
			(end 2.6 3.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2243ea9-533c-42c9-9d74-0818935d3aae")
		)
		(fp_line
			(start 2.6 -0.51)
			(end 2.6 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b8660d9-1c0f-485c-a275-cc05ecde493a")
		)
		(fp_line
			(start 2.6 -3.05)
			(end 2.6 -2.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3525342c-4058-4985-9a7b-64114d525a21")
		)
		(fp_line
			(start 2.6 -5.14)
			(end 2.6 -4.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b7ac2a5-77fb-4bd1-8ebd-a9c96f871ddb")
		)
		(fp_line
			(start -2.6 5.14)
			(end 2.6 5.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45426446-b761-4d86-938f-dfe922137f42")
		)
		(fp_line
			(start -2.6 4.57)
			(end -2.6 5.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31828527-d3e4-4270-929e-a2570b2b175f")
		)
		(fp_line
			(start -2.6 2.03)
			(end -2.6 3.05)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c85ffb0-79c0-4c7d-bc62-c5257d3b9cad")
		)
		(fp_line
			(start -2.6 -0.51)
			(end -2.6 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d9e56e43-35c9-428f-a627-340c943081d6")
		)
		(fp_line
			(start -2.6 -3.05)
			(end -2.6 -2.03)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac0bf232-302c-4ab4-9c0a-288f3f53804f")
		)
		(fp_line
			(start -2.6 -5.14)
			(end 2.6 -5.14)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aabffce1-e759-4aec-91c1-bccfec6a65bb")
		)
		(fp_line
			(start -2.6 -5.14)
			(end -2.6 -4.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "429380fe-e32a-4d00-80e8-452b3a508d53")
		)
		(fp_line
			(start -4.04 -4.57)
			(end -2.6 -4.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0614389-79eb-47c8-8795-3acd45327ced")
		)
		(fp_line
			(start 5.9 5.6)
			(end 5.9 -5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80c34cb0-6b49-453b-9fc6-512a7f280889")
		)
		(fp_line
			(start 5.9 -5.6)
			(end -5.9 -5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fada3b6c-9be9-408b-9721-fa2670900270")
		)
		(fp_line
			(start -5.9 5.6)
			(end 5.9 5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f008c8e-3ffd-4fd0-b35c-25b7591e378b")
		)
		(fp_line
			(start -5.9 -5.6)
			(end -5.9 5.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "afb14573-a8f8-44b6-8571-26b423a2b0bd")
		)
		(fp_line
			(start 3.6 4.13)
			(end 2.54 4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7155f0b8-5740-473d-b293-84f0ee000d31")
		)
		(fp_line
			(start 3.6 3.49)
			(end 3.6 4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1761acc-f677-4198-bf50-793d08999797")
		)
		(fp_line
			(start 3.6 1.59)
			(end 2.54 1.59)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "18dd6732-6511-4225-b214-66fe696c874c")
		)
		(fp_line
			(start 3.6 0.95)
			(end 3.6 1.59)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50a08d86-f795-470e-8e5b-680a252932cd")
		)
		(fp_line
			(start 3.6 -0.95)
			(end 2.54 -0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e60d4a8-f2db-4b54-9d42-d7f7e66cfa24")
		)
		(fp_line
			(start 3.6 -1.59)
			(end 3.6 -0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4e959e0-0849-4738-9f86-2abeda46ca32")
		)
		(fp_line
			(start 3.6 -3.49)
			(end 2.54 -3.49)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e25b040e-3201-4c4e-9dc5-20103783b727")
		)
		(fp_line
			(start 3.6 -4.13)
			(end 3.6 -3.49)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc8440e5-1ee8-46c8-9bd7-0ed669373219")
		)
		(fp_line
			(start 2.54 5.08)
			(end -2.54 5.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7640074-44fa-4703-bd87-34469f548819")
		)
		(fp_line
			(start 2.54 3.49)
			(end 3.6 3.49)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8b93a47-837c-4c3b-b0d6-31e4224a89f6")
		)
		(fp_line
			(start 2.54 0.95)
			(end 3.6 0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2ae0fa1-1eef-4558-8238-156071b5405d")
		)
		(fp_line
			(start 2.54 -1.59)
			(end 3.6 -1.59)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "559c5fb0-7811-4c97-8ac4-9f6bf7c731bf")
		)
		(fp_line
			(start 2.54 -4.13)
			(end 3.6 -4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b411f2a-25f5-4e1e-9b9a-c2f802b5aeb5")
		)
		(fp_line
			(start 2.54 -5.08)
			(end 2.54 5.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae613803-f274-41c4-9430-f970a3df27c6")
		)
		(fp_line
			(start -1.59 -5.08)
			(end 2.54 -5.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "301f3776-011a-4f86-89c3-f638b42408c2")
		)
		(fp_line
			(start -2.54 5.08)
			(end -2.54 -4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7796021-68bf-4e79-a146-f28027ee4ca5")
		)
		(fp_line
			(start -2.54 3.49)
			(end -3.6 3.49)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c9eefa0-9e7a-4fe3-97fa-360b3420b64c")
		)
		(fp_line
			(start -2.54 0.95)
			(end -3.6 0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8672b70b-cad0-4763-8eff-e99170768168")
		)
		(fp_line
			(start -2.54 -1.59)
			(end -3.6 -1.59)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "115d7ba6-7dcc-47b8-8e97-869789c7acc7")
		)
		(fp_line
			(start -2.54 -4.13)
			(end -1.59 -5.08)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "732d5d0d-a12f-49b5-85e4-00cab0d300bf")
		)
		(fp_line
			(start -2.54 -4.13)
			(end -3.6 -4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e635aa7-713c-48c1-a06e-e2bdfef09800")
		)
		(fp_line
			(start -3.6 4.13)
			(end -2.54 4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8ea08791-be26-4034-bfed-d56f8c9b49c3")
		)
		(fp_line
			(start -3.6 3.49)
			(end -3.6 4.13)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d353365a-dc37-411a-a9f9-26ab1c0f9e7a")
		)
		(fp_line
			(start -3.6 1.59)
			(end -2.54 1.59)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02621b4f-9ac7-46aa-8448-be9aef745f47")
		)
		(fp_line
			(start -3.6 0.95)
			(end -3.6 1.59)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4837d5e2-53fa-4c92-af69-6d2e317d5c3e")
		)
		(fp_line
			(start -3.6 -0.95)
			(end -2.54 -0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9abe99f-e701-4ac8-a4d8-6b7b64f4eb96")
		)
		(fp_line
			(start -3.6 -1.59)
			(end -3.6 -0.95)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94258983-9c63-4119-8fcf-df3cdf393d47")
		)
		(fp_line
			(start -3.6 -3.49)
			(end -2.54 -3.49)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b330dece-e31a-4b68-aa75-1ec787104da5")
		)
		(fp_line
			(start -3.6 -4.13)
			(end -3.6 -3.49)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3bfe859f-22ba-4106-9ecd-c94627fb4a4c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "26153cef-ade9-4a2b-82c4-608234bcf6ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -2.525 -3.81 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(J1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e5b1c24d-10ac-45dd-a63c-5d827810167b")
		)
		(pad "2" smd rect
			(at 2.525 -3.81 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "8d8d9f67-bfe6-4665-8cd8-c27c6118c50e")
		)
		(pad "3" smd rect
			(at -2.525 -1.27 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(J1-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(uuid "a5d8148b-667b-4eff-8f52-a29cdfb3086e")
		)
		(pad "4" smd rect
			(at 2.525 -1.27 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(J1-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive")
			(uuid "32cb0d10-7c48-4243-810f-0d7ebb9cf648")
		)
		(pad "5" smd rect
			(at -2.525 1.27 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "D5{slash}A5")
			(pinfunction "Pin_5")
			(pintype "passive")
			(uuid "cc09b9aa-cf61-4e66-b7a9-d268c74ac3c9")
		)
		(pad "6" smd rect
			(at 2.525 1.27 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "5V+")
			(pinfunction "Pin_6")
			(pintype "passive")
			(uuid "5dbe6101-6983-486a-b48f-b266e35fb521")
		)
		(pad "7" smd rect
			(at -2.525 3.81 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "D4{slash}A4")
			(pinfunction "Pin_7")
			(pintype "passive")
			(uuid "90c93f99-0395-4d5e-97d3-332c6c7c3393")
		)
		(pad "8" smd rect
			(at 2.525 3.81 180)
			(size 3.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
			(uuid "e5c2de54-1acc-4a44-91bd-093c2d76ebfe")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical_SMD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 82.5 81.5)
		(end 170.5 123)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "5e42670a-dc99-4f2e-bfe5-4b31348a8ad1")
	)
	(segment
		(start 140.5 117.05)
		(end 138.409 119.141)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "1598f11d-949f-4db0-a909-a58109d4ff1b")
	)
	(segment
		(start 117.31 103.69)
		(end 106.5 114.5)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "25734030-5545-452a-b6ae-1fe665a512d9")
	)
	(segment
		(start 111.141 119.141)
		(end 106.5 114.5)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "26aa4edd-3b59-49b4-b744-ca849d135782")
	)
	(segment
		(start 87.675 104.52)
		(end 87.675 90.14)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "291f976e-49a8-4843-98c8-759cf1c249cf")
	)
	(segment
		(start 140.5 117.05)
		(end 140.5 103.5)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "2931dde2-2a56-434b-938e-35d568b0c309")
	)
	(segment
		(start 118.975 103.69)
		(end 117.31 103.69)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "40ab0141-0d3e-4aae-8914-1a190f7aec07")
	)
	(segment
		(start 106.5 114.5)
		(end 97.655 114.5)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "617315a6-87e4-4387-9ec3-e2b73d578b1f")
	)
	(segment
		(start 140.5 103.5)
		(end 140 103)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "a24dff78-6f71-4297-8cc9-4429d7bd0bd0")
	)
	(segment
		(start 138.409 119.141)
		(end 111.141 119.141)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "bb6683e1-2208-47a9-838d-d9634d8a241b")
	)
	(segment
		(start 97.655 114.5)
		(end 87.675 104.52)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "de391f5d-b298-4d68-b630-9963b5032af7")
	)
	(segment
		(start 87.675 90.14)
		(end 87.845 89.97)
		(width 0.4)
		(layer "F.Cu")
		(net 1)
		(uuid "fb8537ad-92f7-4c08-83b9-a4409cc3ace8")
	)
	(segment
		(start 104.83 89.97)
		(end 92.845 89.97)
		(width 0.4)
		(layer "F.Cu")
		(net 2)
		(uuid "20beebfc-1685-4112-9a51-57f6d66ea4a5")
	)
	(segment
		(start 112.845 90.57)
		(end 105.845 90.57)
		(width 0.4)
		(layer "F.Cu")
		(net 2)
		(uuid "4812f7c9-f1ae-4cec-a2f1-19669af062c5")
	)
	(segment
		(start 105.43 90.57)
		(end 104.83 89.97)
		(width 0.4)
		(layer "F.Cu")
		(net 2)
		(uuid "76649300-cb49-4a84-b8ee-6ad46c783ae9")
	)
	(segment
		(start 105.845 90.57)
		(end 105.43 90.57)
		(width 0.4)
		(layer "F.Cu")
		(net 2)
		(uuid "c754b32b-147e-420a-9583-be7a1aeb22a7")
	)
	(segment
		(start 105.845 102.57)
		(end 94.625 102.57)
		(width 0.4)
		(layer "F.Cu")
		(net 3)
		(uuid "3d053da0-5718-4b9c-a68f-8b9413344ac2")
	)
	(segment
		(start 112.845 102.57)
		(end 105.845 102.57)
		(width 0.4)
		(layer "F.Cu")
		(net 3)
		(uuid "dc380c59-978e-47a0-92cb-ff93e0c1d3cc")
	)
	(segment
		(start 94.625 102.57)
		(end 92.675 104.52)
		(width 0.4)
		(layer "F.Cu")
		(net 3)
		(uuid "f9af5d4c-beed-4422-b6fd-507046606ee7")
	)
	(segment
		(start 144.954 95.064)
		(end 137.46 102.558)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "0f674974-a112-4e98-89fd-f562b98c06d2")
	)
	(segment
		(start 144.954 85.399)
		(end 144.954 95.064)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "113b5046-b2de-431b-a1be-1cdcbcd5b062")
	)
	(segment
		(start 145.254 85.099)
		(end 144.954 85.399)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "34ebd9bf-b0ca-404c-851c-306d8c561f2d")
	)
	(segment
		(start 157.099 85.099)
		(end 145.254 85.099)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "554745d6-c4a4-4969-8f95-34c7c2d0a8db")
	)
	(segment
		(start 137.46 102.558)
		(end 137.46 103)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "a3cce90d-00be-42ad-999b-8217d9210578")
	)
	(segment
		(start 137 117.05)
		(end 137 103.46)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "ac6b6e63-1a0d-4d56-abc4-a3fd3e3b69bd")
	)
	(segment
		(start 158.5 86.5)
		(end 157.099 85.099)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "adb3ef32-da7c-4393-8e9f-7a587fe7a840")
	)
	(segment
		(start 118.975 106.23)
		(end 118.258 106.23)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "b693f90a-c346-462c-b41f-2ab4ac345377")
	)
	(segment
		(start 118.258 106.23)
		(end 111.5 112.988)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "c358cdd7-5f54-42c0-aece-610ce9d4cbb5")
	)
	(segment
		(start 111.5 112.988)
		(end 111.5 114.5)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "cd582a9b-fc77-4d2d-913b-8a0d086f91ab")
	)
	(segment
		(start 134.45 114.5)
		(end 111.5 114.5)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "f3f90ecb-6c3b-4127-8b9d-c6e128f694f5")
	)
	(segment
		(start 137 117.05)
		(end 134.45 114.5)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "fa3dbd56-18e1-45e6-87f1-153c0e79cf45")
	)
	(segment
		(start 137 103.46)
		(end 137.46 103)
		(width 0.4)
		(layer "F.Cu")
		(net 5)
		(uuid "fec8a4e1-1a55-4712-a5fa-faacfde8bf47")
	)
	(segment
		(start 112.845 98.57)
		(end 122.385 89.03)
		(width 0.4)
		(layer "F.Cu")
		(net 6)
		(uuid "04243c86-dcf5-4081-b673-957b54bb1df1")
	)
	(segment
		(start 105.845 98.57)
		(end 112.845 98.57)
		(width 0.4)
		(layer "F.Cu")
		(net 6)
		(uuid "686d26b0-f31f-4a72-a757-19fe0c86b1b5")
	)
	(segment
		(start 122.385 89.03)
		(end 131.11 89.03)
		(width 0.4)
		(layer "F.Cu")
		(net 6)
		(uuid "ca6c2ec9-b711-46b5-b9a3-043664e432b4")
	)
	(segment
		(start 144 117.05)
		(end 144 104.075)
		(width 0.4)
		(layer "F.Cu")
		(net 8)
		(uuid "0ebf0205-a167-43ec-b604-3babbafb01b8")
	)
	(segment
		(start 144 104.075)
		(end 146.345 101.73)
		(width 0.4)
		(layer "F.Cu")
		(net 8)
		(uuid "c0a7c09f-af82-497c-a2d1-c6219be4acbc")
	)
	(segment
		(start 114.01 86.49)
		(end 131.11 86.49)
		(width 0.4)
		(layer "F.Cu")
		(net 9)
		(uuid "23480004-cdc5-41fd-afbf-13ec86ace071")
	)
	(segment
		(start 105.845 86.57)
		(end 112.845 86.57)
		(width 0.4)
		(layer "F.Cu")
		(net 9)
		(uuid "2483c5d9-4356-46d8-9ad1-9134f0722bd0")
	)
	(segment
		(start 113.93 86.57)
		(end 114.01 86.49)
		(width 0.4)
		(layer "F.Cu")
		(net 9)
		(uuid "65f9c2eb-e656-4ec2-9795-053656a6087a")
	)
	(segment
		(start 112.845 86.57)
		(end 113.93 86.57)
		(width 0.4)
		(layer "F.Cu")
		(net 9)
		(uuid "66d7df50-88c4-4574-b184-7deb908af28a")
	)
	(segment
		(start 124.025 103.69)
		(end 124.025 101.793)
		(width 0.4)
		(layer "F.Cu")
		(net 15)
		(uuid "0ffbc89b-98a9-43c3-8f41-37ec2b330b97")
	)
	(segment
		(start 124.025 101.793)
		(end 129.168 96.65)
		(width 0.4)
		(layer "F.Cu")
		(net 15)
		(uuid "22a1f2ff-eb57-469b-a104-f06b3fce097a")
	)
	(segment
		(start 129.168 96.65)
		(end 131.11 96.65)
		(width 0.4)
		(layer "F.Cu")
		(net 15)
		(uuid "2a25ae27-f740-4105-a4a8-18726f395ee2")
	)
	(segment
		(start 132.501 100.581)
		(end 131.11 99.19)
		(width 0.4)
		(layer "F.Cu")
		(net 18)
		(uuid "1b36ac03-0e4a-4895-846e-a273b86c7613")
	)
	(segment
		(start 124.025 106.23)
		(end 129.092 106.23)
		(width 0.4)
		(layer "F.Cu")
		(net 18)
		(uuid "58c0b3f3-fb1f-4bfa-aaa9-107bf2966375")
	)
	(segment
		(start 129.092 106.23)
		(end 132.501 102.821)
		(width 0.4)
		(layer "F.Cu")
		(net 18)
		(uuid "6ef149c1-3efe-455b-9edc-892223acdbbe")
	)
	(segment
		(start 132.501 102.821)
		(end 132.501 100.581)
		(width 0.4)
		(layer "F.Cu")
		(net 18)
		(uuid "af054dc5-b73e-4261-806a-b1aab53f1963")
	)
	(segment
		(start 159.69 99.19)
		(end 146.345 99.19)
		(width 0.4)
		(layer "F.Cu")
		(net 30)
		(uuid "857a3c12-da7d-4984-8509-3797a97da6a8")
	)
	(segment
		(start 161 100)
		(end 160.5 100)
		(width 0.4)
		(layer "F.Cu")
		(net 30)
		(uuid "cafac909-1552-4980-9277-baecd2cc563f")
	)
	(segment
		(start 161 107)
		(end 161 100)
		(width 0.4)
		(layer "F.Cu")
		(net 30)
		(uuid "d9b72718-82b5-48e6-bf44-e9cae91590a7")
	)
	(segment
		(start 160.5 100)
		(end 159.69 99.19)
		(width 0.4)
		(layer "F.Cu")
		(net 30)
		(uuid "dc2e9449-2476-4616-811f-29735483756e")
	)
	(segment
		(start 165 99)
		(end 165.5 98.5)
		(width 0.4)
		(layer "F.Cu")
		(net 33)
		(uuid "30190607-e0d2-4522-9f51-982cc5bb5510")
	)
	(segment
		(start 165 100)
		(end 165 99)
		(width 0.4)
		(layer "F.Cu")
		(net 33)
		(uuid "8758201b-a0d1-4e6a-8713-c3a2cb019113")
	)
	(segment
		(start 165.5 98.5)
		(end 165.5 86.5)
		(width 0.4)
		(layer "F.Cu")
		(net 33)
		(uuid "df626671-ca83-4991-baf9-020946e05e53")
	)
	(segment
		(start 165 107)
		(end 165 100)
		(width 0.4)
		(layer "F.Cu")
		(net 33)
		(uuid "e8f9b15a-cdbd-4559-b1ce-0f116fa3c081")
	)
	(embedded_fonts no)
)
