(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "SimpleLED")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(A1-A0-Pad9)")
	(net 2 "unconnected-(A1-GND-Pad7)")
	(net 3 "unconnected-(A1-+5V-Pad5)")
	(net 4 "unconnected-(A1-A1-Pad10)")
	(net 5 "unconnected-(A1-3V3-Pad4)")
	(net 6 "unconnected-(A1-D13-Pad28)")
	(net 7 "unconnected-(A1-D4-Pad19)")
	(net 8 "unconnected-(A1-A3-Pad12)")
	(net 9 "unconnected-(A1-SDA{slash}A4-Pad13)")
	(net 10 "unconnected-(A1-D9-Pad24)")
	(net 11 "unconnected-(A1-AREF-Pad30)")
	(net 12 "Net-(A1-D2)")
	(net 13 "unconnected-(A1-D7-Pad22)")
	(net 14 "Net-(D1-K)")
	(net 15 "unconnected-(A1-D0{slash}RX-Pad15)")
	(net 16 "unconnected-(A1-SDA{slash}A4-Pad31)")
	(net 17 "unconnected-(A1-D6-Pad21)")
	(net 18 "unconnected-(A1-D5-Pad20)")
	(net 19 "unconnected-(A1-D1{slash}TX-Pad16)")
	(net 20 "unconnected-(A1-SCL{slash}A5-Pad32)")
	(net 21 "unconnected-(A1-A2-Pad11)")
	(net 22 "Net-(BT1--)")
	(net 23 "Net-(A1-VIN)")
	(net 24 "unconnected-(A1-D11-Pad26)")
	(net 25 "unconnected-(A1-IOREF-Pad2)")
	(net 26 "unconnected-(A1-~{RESET}-Pad3)")
	(net 27 "unconnected-(A1-D3-Pad18)")
	(net 28 "unconnected-(A1-D10-Pad25)")
	(net 29 "unconnected-(A1-NC-Pad1)")
	(net 30 "unconnected-(A1-D8-Pad23)")
	(net 31 "unconnected-(A1-SCL{slash}A5-Pad14)")
	(net 32 "unconnected-(A1-D12-Pad27)")
	(net 33 "Net-(BT1-+)")
	(net 34 "Net-(D1-A)")
	(footprint "Battery:BatteryHolder_LINX_BAT-HLD-012-SMT"
		(layer "F.Cu")
		(uuid "4d7bcd97-f89d-40f0-ba4a-659e2cb76fc0")
		(at 149.5 65.6 -90)
		(descr "SMT battery holder for CR1216/1220/1225, https://linxtechnologies.com/wp/wp-content/uploads/bat-hld-012-smt.pdf")
		(tags "battery holder coin cell cr1216 cr1220 cr1225")
		(property "Reference" "BT1"
			(at 0 6 90)
			(layer "F.SilkS")
			(uuid "f3ceb9c8-3ba3-4522-a2ef-aa46909d30ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3V"
			(at 16 3 90)
			(layer "F.Fab")
			(uuid "7737f373-5250-4d9a-9b1a-28b9c30b3880")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9fa9c688-0cf0-475c-8298-27d4bbbbf310")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f213190-27fd-4c50-bcf4-ad5093a1de6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "V"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac66c2da-12b0-40fb-95d6-dd96016bba56")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "DC"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eca0a447-3d79-4395-8049-044152b2b0f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "255c9881-c415-4309-9f58-29745ec93688")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/7cb6659a-7595-4e1c-ab07-84d25e229d9c")
		(sheetname "/")
		(sheetfile "03_KiCad_simpleLED.kicad_sch")
		(attr smd)
		(fp_line
			(start -6.55 2.85)
			(end -5.4 4.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19dff1c8-3e15-4030-a5ac-ab230b71d1a6")
		)
		(fp_line
			(start 6.55 2.85)
			(end 5.4 4.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3dff7a87-5628-4f01-8a9f-233c4031e6a2")
		)
		(fp_line
			(start -6.55 -2.75)
			(end -4.9 -4.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d30963a-9f64-4730-90b0-26148b11032b")
		)
		(fp_line
			(start -4.9 -4.4)
			(end -3 -4.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92ab2f41-801c-4693-82e5-8af33f71c17a")
		)
		(fp_line
			(start 4.9 -4.4)
			(end 6.55 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e520a18-51e2-4236-a914-2db9f016c3f2")
		)
		(fp_line
			(start 4.9 -4.4)
			(end 3 -4.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95c21f63-7c7b-4473-a063-834aada11656")
		)
		(fp_arc
			(start -2.504098 4.697607)
			(mid -4.031094 4.908816)
			(end -5.4 4.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a55352f-910a-40df-9b8f-b25e310c1703")
		)
		(fp_arc
			(start 5.4 4.2)
			(mid 4.029781 4.909041)
			(end 2.501694 4.696459)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8238ec5-e160-4a8a-a1f0-3e06e2d04109")
		)
		(fp_line
			(start -3.55 6.75)
			(end 3.55 6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aad11004-b278-4f02-b201-178a76d9af49")
		)
		(fp_line
			(start -3.55 6.75)
			(end -7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8773fd5e-6e5c-4ed2-b041-65a741f14cb8")
		)
		(fp_line
			(start 3.55 6.75)
			(end 7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f58dd48-9a76-427f-a4e1-47cd428f8d45")
		)
		(fp_line
			(start -9.35 3.05)
			(end -7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6768bb9-323f-44aa-a32e-93445dc45117")
		)
		(fp_line
			(start -9.35 3.05)
			(end -9.35 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e73a3ac5-09d6-439e-a8cc-332c055e54ae")
		)
		(fp_line
			(start 9.35 3.05)
			(end 7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f014886-203e-43db-94c4-549c3867a13b")
		)
		(fp_line
			(start -9.35 -3.05)
			(end -7.25 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6c7d05d-4803-4470-a353-c66cab7823de")
		)
		(fp_line
			(start -7.25 -3.05)
			(end -3.55 -6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dac61f44-ec79-4ffd-b9fe-48b698e28544")
		)
		(fp_line
			(start 7.25 -3.05)
			(end 9.35 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba2a7318-fff0-4d03-b591-8b0e5c54542d")
		)
		(fp_line
			(start 9.35 -3.05)
			(end 9.35 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98038ba0-e9cd-458d-83d1-b90ca8fc500b")
		)
		(fp_line
			(start -3.55 -6.75)
			(end 3.55 -6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b0ca8589-39ed-4424-baf8-dc07da2dbe5e")
		)
		(fp_line
			(start 3.55 -6.75)
			(end 7.25 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a20627a-a9de-406a-aef4-fec6bdd81b7e")
		)
		(fp_line
			(start -6.75 2.85)
			(end -6.55 2.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d13836f-0aff-4d08-83ab-ac466f7efcff")
		)
		(fp_line
			(start -6.75 2.85)
			(end -6.75 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ba5fb2f-946b-497b-b468-35b24e34d812")
		)
		(fp_line
			(start -6.55 2.85)
			(end -5.4 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a92b1bd-06b4-456d-b69f-9f95af0c07a0")
		)
		(fp_line
			(start -6.55 2.85)
			(end -6.55 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45b90349-a135-42d7-b952-08b0409b5865")
		)
		(fp_line
			(start 6.55 2.85)
			(end 5.4 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eedf1463-457b-42d9-97f0-acdf910de369")
		)
		(fp_line
			(start 6.55 2.85)
			(end 6.55 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca3570b4-0fd6-4df1-838d-cd2d65d70cad")
		)
		(fp_line
			(start 6.75 2.85)
			(end 6.55 2.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbaa00f3-13c0-4489-a41e-25731b389507")
		)
		(fp_line
			(start 6.75 2.85)
			(end 6.75 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "834f24c2-59a5-44f2-a1e3-f4115f00f940")
		)
		(fp_line
			(start -7.65 2.55)
			(end -6.75 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5a7ca05e-2ca8-45b5-a5d5-be6be62a6890")
		)
		(fp_line
			(start 6.75 2.55)
			(end 7.65 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b43fa19-d755-44b6-9b48-417bfc658ea1")
		)
		(fp_line
			(start 7.65 2.55)
			(end 7.65 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98481637-d88b-4d65-a3b9-f211bb4b4b1b")
		)
		(fp_line
			(start -7.65 0.55)
			(end -7.65 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36b9e872-366c-4b9b-9fd1-35321284cc88")
		)
		(fp_line
			(start -6.75 0.55)
			(end -7.65 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6a7b674-9f67-4e9b-acc5-5cc02ddd4372")
		)
		(fp_line
			(start 7.65 0.55)
			(end 6.75 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c851e79a-0b34-4036-be1e-44f9754113fb")
		)
		(fp_line
			(start -7.65 -0.55)
			(end -6.75 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1fe5db88-ea7e-4838-a293-03549bf564a7")
		)
		(fp_line
			(start 6.75 -0.55)
			(end 7.65 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7c04331-5b28-4e76-9d97-c5f74a322642")
		)
		(fp_line
			(start 7.65 -0.55)
			(end 7.65 -2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f93723af-7d10-4a3f-83b2-963b8ae2c226")
		)
		(fp_line
			(start -7.65 -2.55)
			(end -7.65 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "568670eb-f59f-4fcd-8017-14f851e54126")
		)
		(fp_line
			(start -7.65 -2.55)
			(end -6.75 -2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28f619ae-52cc-4994-8195-2e15e11c060a")
		)
		(fp_line
			(start 7.65 -2.55)
			(end 6.75 -2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb6cf68d-7b75-41ab-a928-eb2f9a8daf82")
		)
		(fp_line
			(start -6.75 -2.75)
			(end -6.55 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d6a2f18-5dd2-4ea1-8a15-5524c44575d5")
		)
		(fp_line
			(start -6.55 -2.75)
			(end -6.7 -2.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "67470f51-b907-40a7-9efc-07153d587dde")
		)
		(fp_line
			(start -6.55 -2.75)
			(end -4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46e772f2-e790-4fc8-ac60-50b278aecbbf")
		)
		(fp_line
			(start 6.55 -2.75)
			(end 6.75 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9dc743b6-9c21-4699-814e-39df265eedad")
		)
		(fp_line
			(start 6.55 -2.75)
			(end 6.7 -2.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d9b2359-da2e-41b2-8439-a83bcbf4336d")
		)
		(fp_line
			(start 6.55 -2.75)
			(end 4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8335764c-b2a5-48c6-89ed-d44548142d5f")
		)
		(fp_line
			(start -6.7 -2.9)
			(end -5.05 -4.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fa4dde75-4296-4acb-8eea-520f7719318e")
		)
		(fp_line
			(start 6.7 -2.9)
			(end 5.05 -4.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cae853fd-69b0-4c24-a256-2935060de91a")
		)
		(fp_line
			(start 4.9 -4.4)
			(end -4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a75f61ee-1686-414a-9190-c234a820519c")
		)
		(fp_line
			(start -5.05 -4.55)
			(end -4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "51e8ef06-65e5-4ec6-b47f-9c087f143295")
		)
		(fp_line
			(start 5.05 -4.55)
			(end 4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cd1110f-6a87-41c7-9c79-4926824ea6e1")
		)
		(fp_arc
			(start -1.8 4.2)
			(mid -3.6 4.945584)
			(end -5.4 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0bcc76d-d5b6-46dc-89e2-579a51ad4472")
		)
		(fp_arc
			(start -1.8 4.2)
			(mid 0 3.454416)
			(end 1.8 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8299294-fbc9-4449-a72a-b7985c98b5e5")
		)
		(fp_arc
			(start 5.4 4.2)
			(mid 3.6 4.945584)
			(end 1.8 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2dc3512d-ea4a-4cae-8aa9-1616a19b4fa9")
		)
		(fp_circle
			(center 0 0)
			(end -6.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "f5c23262-3057-48a4-a63d-a3cf5f887550")
		)
		(fp_text user "${REFERENCE}"
			(at 16 5.5 90)
			(layer "F.Fab")
			(uuid "d6783f81-c84f-4090-8c9c-fa047edd664c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -7.6 0 270)
			(size 2.5 5.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "8edcf580-c5a2-475a-af6d-15b09af18ff1")
		)
		(pad "1" smd rect
			(at 7.6 0 270)
			(size 2.5 5.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "3eafcf37-1210-4a8c-a8ff-fc2863305f94")
		)
		(pad "2" smd circle
			(at 0 0 270)
			(size 10.2 10.2)
			(layers "F.Cu" "F.Mask")
			(net 22 "Net-(BT1--)")
			(pinfunction "-")
			(pintype "passive")
			(uuid "d33a4b17-3259-4fcb-ad24-4aab9a336081")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_LINX_BAT-HLD-012-SMT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0201_0603Metric"
		(layer "F.Cu")
		(uuid "5e34506a-2b93-4b47-bd17-ef2f4649d1f8")
		(at 139.345 137)
		(descr "LED SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -5.5 -0.5 0)
			(layer "F.SilkS")
			(uuid "85e9ebb1-7123-4912-977f-9c63cbe3c8c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3V"
			(at -8.845 0 0)
			(layer "F.Fab")
			(uuid "e956aa46-b760-45e6-b9a0-3bbbd5a44ccb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f90f8f56-420a-4a85-81c9-de2ecc4e07ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "71b8be44-fa32-45af-acc9-ef94a7be0c69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc796a6a-89fb-4108-a955-3f7fffeac81d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(path "/2b6159f5-067f-4d75-a170-61601bd12f51")
		(sheetname "/")
		(sheetfile "03_KiCad_simpleLED.kicad_sch")
		(attr smd)
		(fp_circle
			(center -0.86 0)
			(end -0.81 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "aa3ee7ec-0d11-496d-ac34-c4b3017d9051")
		)
		(fp_rect
			(start -0.7 -0.35)
			(end 0.7 0.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a42f5c36-f060-4372-85a5-1bb86b362f28")
		)
		(fp_line
			(start -0.2 0.15)
			(end -0.2 -0.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0002b963-45cd-409b-ba64-873d64ecc3c1")
		)
		(fp_line
			(start -0.1 0.15)
			(end -0.1 -0.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76759cc5-ab39-4851-a243-1d81bcf0618f")
		)
		(fp_rect
			(start -0.3 -0.15)
			(end 0.3 0.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "afdbe62a-63cc-40f7-8d69-423fd658e639")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
			(uuid "97dc8f03-bac6-4778-874a-3c3a4d2734e7")
			(effects
				(font
					(size 0.25 0.25)
					(thickness 0.04)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "b0fa7079-ebf4-4b28-9f48-b96dcc2b459c")
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "5d4aa398-e503-4294-a119-c45fc3aef2bd")
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "761de7ab-6e71-449d-b72f-a431aa3806e8")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "887f380a-9fa2-4113-bab9-7b62df58ae60")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Battery:BatteryHolder_LINX_BAT-HLD-012-SMT"
		(layer "F.Cu")
		(uuid "5fdfecde-b859-40f7-9a59-4d021b2e4f51")
		(at 169.5 65.6 -90)
		(descr "SMT battery holder for CR1216/1220/1225, https://linxtechnologies.com/wp/wp-content/uploads/bat-hld-012-smt.pdf")
		(tags "battery holder coin cell cr1216 cr1220 cr1225")
		(property "Reference" "BT2"
			(at 0 6 90)
			(layer "F.SilkS")
			(uuid "a958a42a-6956-4d29-9deb-42dddb355df0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "3V"
			(at 0 -7 90)
			(layer "F.Fab")
			(uuid "a445d2a2-e54d-4d44-b9b9-c976c7eb647e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1514badf-c536-4bb0-84a2-0a499169d321")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "43aadede-0e17-460f-a516-f0e3fd22f90a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" "V"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "362fba41-7470-4dcb-bbd0-78894730db8e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Type" "DC"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbcebb75-ab71-4113-bb0d-78809ff2d303")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f08034a-29e3-406f-b751-b7bd6c0bf25f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/b9eeb9b2-5e5b-4182-9b53-e69ad188688d")
		(sheetname "/")
		(sheetfile "03_KiCad_simpleLED.kicad_sch")
		(attr smd)
		(fp_line
			(start -6.55 2.85)
			(end -5.4 4.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48ef04a9-fe17-43dd-9a77-9cc340230d63")
		)
		(fp_line
			(start 6.55 2.85)
			(end 5.4 4.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0c80fcc-5275-4a98-8374-d0e367fbb11e")
		)
		(fp_line
			(start -6.55 -2.75)
			(end -4.9 -4.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97a24de9-6499-434d-bdab-7bcd67a50304")
		)
		(fp_line
			(start -4.9 -4.4)
			(end -3 -4.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3fe1743e-c935-4b98-9266-fe18f04f403f")
		)
		(fp_line
			(start 4.9 -4.4)
			(end 6.55 -2.75)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a28b47d-c530-408d-8509-d2463968803a")
		)
		(fp_line
			(start 4.9 -4.4)
			(end 3 -4.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2165090-b49d-43dc-b026-2eaf0033d367")
		)
		(fp_arc
			(start -2.504098 4.697607)
			(mid -4.031094 4.908816)
			(end -5.4 4.2)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5170f437-9ef7-4a37-9f4c-32bc5e49b494")
		)
		(fp_arc
			(start 5.4 4.2)
			(mid 4.029781 4.909041)
			(end 2.501694 4.696459)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1792bfa3-f7ac-49b8-bfb4-680b7b04e899")
		)
		(fp_line
			(start -3.55 6.75)
			(end 3.55 6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60ef7dcb-2ff7-4666-93e2-20dda58eda4e")
		)
		(fp_line
			(start -3.55 6.75)
			(end -7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd220ceb-89b4-44f5-b408-dbbcfd516ec7")
		)
		(fp_line
			(start 3.55 6.75)
			(end 7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e5a24c2-b848-4d9d-ae49-a69d35db5838")
		)
		(fp_line
			(start -9.35 3.05)
			(end -7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1f4cca0d-218c-4c58-9f10-c2bde1cddc2c")
		)
		(fp_line
			(start -9.35 3.05)
			(end -9.35 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c56b2b18-1085-404a-b71f-94fb5ece2744")
		)
		(fp_line
			(start 9.35 3.05)
			(end 7.25 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5b2dde5-e1a9-4771-8a04-5f8a0bd9d752")
		)
		(fp_line
			(start -9.35 -3.05)
			(end -7.25 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "665fa2b3-22f5-4dd3-827c-ad3cb4bf1bd8")
		)
		(fp_line
			(start -7.25 -3.05)
			(end -3.55 -6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dde5d721-9465-4251-8cb3-0ddcf3599119")
		)
		(fp_line
			(start 7.25 -3.05)
			(end 9.35 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e55af2ef-3e44-4363-bf48-50d4a73a0534")
		)
		(fp_line
			(start 9.35 -3.05)
			(end 9.35 3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6a3f7166-c419-42c1-aee6-73703daa534b")
		)
		(fp_line
			(start -3.55 -6.75)
			(end 3.55 -6.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5539d922-82d7-440a-ba01-e4dbeaba756f")
		)
		(fp_line
			(start 3.55 -6.75)
			(end 7.25 -3.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5168884c-8a9d-4edb-bc2d-81e56fc52871")
		)
		(fp_line
			(start -6.75 2.85)
			(end -6.55 2.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b98c6c7a-ab00-4869-a9ac-e83da19d2a55")
		)
		(fp_line
			(start -6.75 2.85)
			(end -6.75 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52d8d690-4ca7-48ce-b443-4f977c067edf")
		)
		(fp_line
			(start -6.55 2.85)
			(end -5.4 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8689b94f-9cf8-4564-a932-81da38f7af60")
		)
		(fp_line
			(start -6.55 2.85)
			(end -6.55 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8c4de47-4d58-4ec0-94b3-d6beecca24a8")
		)
		(fp_line
			(start 6.55 2.85)
			(end 5.4 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8627b437-1c28-47f9-8a90-b7c9982b5ee6")
		)
		(fp_line
			(start 6.55 2.85)
			(end 6.55 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0b93ac6-1557-48d4-b268-1d674f0a1a6c")
		)
		(fp_line
			(start 6.75 2.85)
			(end 6.55 2.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77f6a1bc-c7cc-4cd5-ba39-424d3e662bbf")
		)
		(fp_line
			(start 6.75 2.85)
			(end 6.75 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd09f03f-39fe-4ac3-9998-256958d99487")
		)
		(fp_line
			(start -7.65 2.55)
			(end -6.75 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16d6fb71-b425-4a24-9a99-f9b2700bcf69")
		)
		(fp_line
			(start 6.75 2.55)
			(end 7.65 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d823e67-025a-490e-b123-29cbfac5a63f")
		)
		(fp_line
			(start 7.65 2.55)
			(end 7.65 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57a4efd1-faf6-4d9e-b982-f85c987c9929")
		)
		(fp_line
			(start -7.65 0.55)
			(end -7.65 2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87bb9a99-9341-4b6f-a4b5-17a54a8dc861")
		)
		(fp_line
			(start -6.75 0.55)
			(end -7.65 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c3065ee-3166-4cd1-b7db-552ad5632b18")
		)
		(fp_line
			(start 7.65 0.55)
			(end 6.75 0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0fe4bbed-8a53-4346-b336-f87f5ed56144")
		)
		(fp_line
			(start -7.65 -0.55)
			(end -6.75 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6b5c0f50-e4f5-4e9f-94a1-3146947314d7")
		)
		(fp_line
			(start 6.75 -0.55)
			(end 7.65 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46424a3d-6508-4a62-a88a-2d966a5343a5")
		)
		(fp_line
			(start 7.65 -0.55)
			(end 7.65 -2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea53550b-158b-48fa-a6f0-85fc257295e2")
		)
		(fp_line
			(start -7.65 -2.55)
			(end -7.65 -0.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed33ffbf-cf7f-4954-99bb-b942cea7ff30")
		)
		(fp_line
			(start -7.65 -2.55)
			(end -6.75 -2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69f52952-41d7-4edf-95ad-5d40e9c46c83")
		)
		(fp_line
			(start 7.65 -2.55)
			(end 6.75 -2.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf17e19d-37a1-49b7-b9e6-9e49dc3b095d")
		)
		(fp_line
			(start -6.75 -2.75)
			(end -6.55 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3361af2-b5ea-4747-abb4-34fb6aecf8e4")
		)
		(fp_line
			(start -6.55 -2.75)
			(end -6.7 -2.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2d0a62e7-00e2-4ac4-8b39-7b14fa3aaf77")
		)
		(fp_line
			(start -6.55 -2.75)
			(end -4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79d4a1af-53a7-44ed-904b-b567e5ce8051")
		)
		(fp_line
			(start 6.55 -2.75)
			(end 6.75 -2.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ffb0893-72f3-4b90-8842-382a3c72c99e")
		)
		(fp_line
			(start 6.55 -2.75)
			(end 6.7 -2.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89b8eb40-939d-4619-a870-579e491e6a46")
		)
		(fp_line
			(start 6.55 -2.75)
			(end 4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23537269-4f36-4913-8e5f-a36c9a3e9a60")
		)
		(fp_line
			(start -6.7 -2.9)
			(end -5.05 -4.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c759a19-2b1d-4a1e-b285-640ab80ec476")
		)
		(fp_line
			(start 6.7 -2.9)
			(end 5.05 -4.55)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a16c732-d7c4-42e1-8fbc-4260e2a23bc4")
		)
		(fp_line
			(start 4.9 -4.4)
			(end -4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98b84ffa-e05c-4b98-add3-e363b1ca301a")
		)
		(fp_line
			(start -5.05 -4.55)
			(end -4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d7eba09-e9b8-41eb-bb6c-971e6920e645")
		)
		(fp_line
			(start 5.05 -4.55)
			(end 4.9 -4.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d79e192e-8fa4-43cb-83c2-9c170bb3f8fd")
		)
		(fp_arc
			(start -1.8 4.2)
			(mid -3.6 4.945584)
			(end -5.4 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b6e72e6-f0f7-4599-866b-d79d07821ab5")
		)
		(fp_arc
			(start -1.8 4.2)
			(mid 0 3.454416)
			(end 1.8 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac5b0285-3842-4f2c-9c02-a648cbcbffa1")
		)
		(fp_arc
			(start 5.4 4.2)
			(mid 3.6 4.945584)
			(end 1.8 4.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6580b78-5a53-4ac6-a32e-6f9b0463022e")
		)
		(fp_circle
			(center 0 0)
			(end -6.25 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "bbc783e8-c9be-42e6-be44-3c0e076c53c7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c9363a06-dfd7-4a4b-bfef-83c0cf7c659e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd rect
			(at -7.6 0 270)
			(size 2.5 5.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(A1-VIN)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "44476d8d-9031-40d3-9686-371d93bbc353")
		)
		(pad "1" smd rect
			(at 7.6 0 270)
			(size 2.5 5.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(A1-VIN)")
			(pinfunction "+")
			(pintype "passive")
			(uuid "7931027a-fb80-4768-bead-0d30cb73abb3")
		)
		(pad "2" smd circle
			(at 0 0 270)
			(size 10.2 10.2)
			(layers "F.Cu" "F.Mask")
			(net 33 "Net-(BT1-+)")
			(pinfunction "-")
			(pintype "passive")
			(uuid "a998d12c-a616-46c7-b8fb-ed56b4c68563")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_LINX_BAT-HLD-012-SMT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Arduino_UNO_R3"
		(layer "F.Cu")
		(uuid "6382654e-b2ab-4b1e-9c5b-c17e1502ee0c")
		(at 140.325 80.37)
		(descr "Arduino UNO R3, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
		(tags "Arduino UNO R3")
		(property "Reference" "A1"
			(at 1.27 -3.81 180)
			(layer "F.SilkS")
			(uuid "f4aaa0ee-96cf-4a12-9e84-3d10f6c2a5b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Arduino_UNO_R3"
			(at -6.825 6.63 0)
			(layer "F.Fab")
			(uuid "465d8142-d454-4c19-92f7-b1f34323b63f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "962e7127-813a-4c1b-bb88-ddcd32282c3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Arduino UNO Microcontroller Module, release 3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "48399698-9bca-45d5-becb-c175780e691c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Arduino*UNO*R3*")
		(path "/f4fee747-79d8-493a-bac1-37390036be09")
		(sheetname "/")
		(sheetfile "03_KiCad_simpleLED.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -34.42 29.72)
			(end -34.42 41.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97cc0321-a3a8-4ea1-9c7f-f52cb02aadf2")
		)
		(fp_line
			(start -34.42 41.4)
			(end -28.07 41.4)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f44b5ab8-126a-4613-a6eb-955e1d66cde0")
		)
		(fp_line
			(start -29.97 0.51)
			(end -29.97 9.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec0eadda-7a78-4560-9b09-e57538cea7b0")
		)
		(fp_line
			(start -29.97 9.65)
			(end -28.07 9.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a6d9040-bf7e-4b9a-9ea8-ead781d4e27e")
		)
		(fp_line
			(start -28.07 -2.67)
			(end -28.07 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8218fda3-3d1d-4403-a7ce-ab1e17da87df")
		)
		(fp_line
			(start -28.07 0.51)
			(end -29.97 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb02f6f9-b378-4b17-8630-c06715728e63")
		)
		(fp_line
			(start -28.07 9.65)
			(end -28.07 29.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09992cb2-bcbf-45fe-8be2-8a1cb12f32ea")
		)
		(fp_line
			(start -28.07 29.72)
			(end -34.42 29.72)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "623485e4-67e2-44f2-ba48-c40a840f5765")
		)
		(fp_line
			(start -28.07 41.4)
			(end -28.07 50.93)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d66f2d5-b073-4a67-912b-17cae8ac062f")
		)
		(fp_line
			(start -28.07 50.93)
			(end 36.58 50.93)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a1c7eb6-74d6-4618-ae2f-d1fa86526d39")
		)
		(fp_line
			(start 36.58 50.93)
			(end 38.23 49.28)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "601a14d3-05f2-4bfd-bb85-f78d402478ce")
		)
		(fp_line
			(start 38.23 -2.67)
			(end -28.07 -2.67)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7006bd4b-1023-4a1e-948e-fd726d160995")
		)
		(fp_line
			(start 38.23 0)
			(end 38.23 -2.67)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35bf6d37-3686-4934-8c63-15de39086f30")
		)
		(fp_line
			(start 38.23 37.85)
			(end 40.77 35.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a508a0f2-71d9-4066-9932-5b57d85ec859")
		)
		(fp_line
			(start 38.23 49.28)
			(end 38.23 37.85)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51a568aa-28cd-4fa5-8338-c6279441707f")
		)
		(fp_line
			(start 40.77 2.54)
			(end 38.23 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "713a5f53-e1ca-41a3-973e-d4fedd934fdd")
		)
		(fp_line
			(start 40.77 35.31)
			(end 40.77 2.54)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6e55d2e-b869-48d7-bba5-c995382aa12b")
		)
		(fp_line
			(start -34.54 29.59)
			(end -28.19 29.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "957184d4-ea43-44f3-b5a3-f77339ab5161")
		)
		(fp_line
			(start -34.54 41.53)
			(end -34.54 29.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3689f0ab-fa8e-4431-b287-fac62e9e69d7")
		)
		(fp_line
			(start -30.1 0.38)
			(end -28.19 0.38)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6690618-acab-431f-9c0c-ae7b9ba11dd1")
		)
		(fp_line
			(start -30.1 9.78)
			(end -30.1 0.38)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38138954-0262-4747-b22e-fdfee6d4dbd9")
		)
		(fp_line
			(start -28.19 -2.79)
			(end 38.35 -2.79)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15a7578e-3416-481b-87a5-25f0472225d6")
		)
		(fp_line
			(start -28.19 0.38)
			(end -28.19 -2.79)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5e45642-57e1-482e-a070-cbd0320378b9")
		)
		(fp_line
			(start -28.19 9.78)
			(end -30.1 9.78)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90482ce4-f7dc-4018-85ca-ab4602ee9a5b")
		)
		(fp_line
			(start -28.19 29.59)
			(end -28.19 9.78)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17b60055-0dff-4310-84a8-2a8931325595")
		)
		(fp_line
			(start -28.19 41.53)
			(end -34.54 41.53)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4bca3440-453a-49ad-8be0-4cbd2b9e3800")
		)
		(fp_line
			(start -28.19 51.05)
			(end -28.19 41.53)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db36797e-e94f-4c7a-87da-9c173e44b061")
		)
		(fp_line
			(start 36.58 51.05)
			(end -28.19 51.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b0127df5-29ca-4d66-a836-9046f70761a6")
		)
		(fp_line
			(start 38.35 -2.79)
			(end 38.35 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0f168d2d-023f-4573-9189-78b1797fc42d")
		)
		(fp_line
			(start 38.35 0)
			(end 40.89 2.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "428077f4-2cc7-4b79-9faf-fdc645b1f9dc")
		)
		(fp_line
			(start 38.35 37.85)
			(end 38.35 49.28)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4a8de79-ee2f-4595-96ca-97553f3856f8")
		)
		(fp_line
			(start 38.35 49.28)
			(end 36.58 51.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97790dec-e4ca-42d1-b0e6-92dfecd5c040")
		)
		(fp_line
			(start 40.89 2.54)
			(end 40.89 35.31)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "646e9df3-e089-4182-8d38-b8b1271d8cb2")
		)
		(fp_line
			(start 40.89 35.31)
			(end 38.35 37.85)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "da38200d-254b-4871-95f9-b8ade3848c66")
		)
		(fp_line
			(start -34.29 29.84)
			(end -18.41 29.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f979cedc-60ff-47bc-b3cb-f250578e87cf")
		)
		(fp_line
			(start -34.29 41.27)
			(end -34.29 29.84)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dde2981f-1904-4d41-bd43-8767388c9dad")
		)
		(fp_line
			(start -29.84 0.64)
			(end -16.51 0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5359e25a-f0be-4fd1-b219-6924e1b502b8")
		)
		(fp_line
			(start -29.84 9.53)
			(end -29.84 0.64)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4ce18a4-749a-4f7e-a6a3-d565c757659d")
		)
		(fp_line
			(start -27.94 -2.54)
			(end 38.1 -2.54)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9402476c-78a7-4db5-b6b8-89e86c389689")
		)
		(fp_line
			(start -27.94 50.8)
			(end -27.94 -2.54)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "acc2f610-d21b-4082-b722-22b2201411da")
		)
		(fp_line
			(start -18.41 29.84)
			(end -18.41 41.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50d8a845-36d2-4473-8772-d728472e9df1")
		)
		(fp_line
			(start -18.41 41.27)
			(end -34.29 41.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89fe1c34-4f22-477d-9d9a-ebef37d33251")
		)
		(fp_line
			(start -16.51 0.64)
			(end -16.51 9.53)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "123bdf8e-37e3-4841-868f-ea71c7f14640")
		)
		(fp_line
			(start -16.51 9.53)
			(end -29.84 9.53)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c124d83d-1153-4555-ab66-7ead238d23ca")
		)
		(fp_line
			(start 36.58 50.8)
			(end -27.94 50.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59b27b6f-05ab-431b-ab00-66bf6af865a3")
		)
		(fp_line
			(start 38.1 -2.54)
			(end 38.1 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e31e2bdf-4252-416b-a1c3-5722eb203136")
		)
		(fp_line
			(start 38.1 0)
			(end 40.64 2.54)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e23644b-295c-401c-8c5d-ce21501c75f6")
		)
		(fp_line
			(start 38.1 37.85)
			(end 38.1 49.28)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7747ff15-908a-40ce-a0da-4b333f0019d3")
		)
		(fp_line
			(start 38.1 49.28)
			(end 36.58 50.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c25d2504-cc47-4151-8601-ed570620733b")
		)
		(fp_line
			(start 40.64 2.54)
			(end 40.64 35.31)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64245970-9053-4dde-af35-e68d48959b37")
		)
		(fp_line
			(start 40.64 35.31)
			(end 38.1 37.85)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8d284b4-d77e-4dbd-a0a5-6367479c2ce7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 20.32 180)
			(layer "F.Fab")
			(uuid "3a27bb99-de18-48cd-83bb-54a17a01cfa3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "d8750182-b3ac-45e4-aae4-7167203a27ae")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(A1-IOREF-Pad2)")
			(pinfunction "IOREF")
			(pintype "output")
			(uuid "cb4b89a9-6d8c-4b56-b43e-71fa60345732")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(A1-~{RESET}-Pad3)")
			(pinfunction "~{RESET}")
			(pintype "input")
			(uuid "cc79fac1-4f81-420e-b30e-3dcc7de0b6fb")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(A1-3V3-Pad4)")
			(pinfunction "3V3")
			(pintype "power_out")
			(uuid "26eaefb7-518e-480b-a91f-51e8815f1520")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(A1-+5V-Pad5)")
			(pinfunction "+5V")
			(pintype "power_out")
			(uuid "0f00de43-081e-44fe-bc8e-f43cd57d631a")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(BT1--)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "b5b1571a-09d6-42a2-8293-3bec34f6eb67")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(A1-GND-Pad7)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "058eb810-674a-4601-a76d-b8c259060f40")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(A1-VIN)")
			(pinfunction "VIN")
			(pintype "power_in")
			(uuid "b95da396-88ee-446e-9e6f-6c6ab646e42d")
		)
		(pad "9" thru_hole oval
			(at 22.86 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(A1-A0-Pad9)")
			(pinfunction "A0")
			(pintype "bidirectional")
			(uuid "05819811-349a-4a75-9b0e-5d8013257207")
		)
		(pad "10" thru_hole oval
			(at 25.4 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-A1-Pad10)")
			(pinfunction "A1")
			(pintype "bidirectional")
			(uuid "2431ec40-017c-4f7f-bf9d-89e0d73610de")
		)
		(pad "11" thru_hole oval
			(at 27.94 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(A1-A2-Pad11)")
			(pinfunction "A2")
			(pintype "bidirectional")
			(uuid "b539099b-3d97-4b36-a463-3099f9d96658")
		)
		(pad "12" thru_hole oval
			(at 30.48 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(A1-A3-Pad12)")
			(pinfunction "A3")
			(pintype "bidirectional")
			(uuid "490c7fb2-5772-4d0f-8d8c-ef9e2bd6ddac")
		)
		(pad "13" thru_hole oval
			(at 33.02 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(A1-SDA{slash}A4-Pad13)")
			(pinfunction "SDA/A4")
			(pintype "bidirectional")
			(uuid "4a1c31b7-f24e-45dc-9373-2c286d7c8ab0")
		)
		(pad "14" thru_hole oval
			(at 35.56 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(A1-SCL{slash}A5-Pad14)")
			(pinfunction "SCL/A5")
			(pintype "bidirectional")
			(uuid "ed1ce55c-ccfe-48ba-bad0-7ff76bfd67b0")
		)
		(pad "15" thru_hole oval
			(at 35.56 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(A1-D0{slash}RX-Pad15)")
			(pinfunction "D0/RX")
			(pintype "bidirectional")
			(uuid "76c70642-b0aa-4f25-b52c-41bd1345617b")
		)
		(pad "16" thru_hole oval
			(at 33.02 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(A1-D1{slash}TX-Pad16)")
			(pinfunction "D1/TX")
			(pintype "bidirectional")
			(uuid "a895333f-9a01-48a2-8abe-777799996a40")
		)
		(pad "17" thru_hole oval
			(at 30.48 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(A1-D2)")
			(pinfunction "D2")
			(pintype "bidirectional")
			(uuid "5d786b39-19f3-4f59-80d0-a0eea64f5eec")
		)
		(pad "18" thru_hole oval
			(at 27.94 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(A1-D3-Pad18)")
			(pinfunction "D3")
			(pintype "bidirectional")
			(uuid "d06d3628-d1ed-44e4-a732-4a921dd99407")
		)
		(pad "19" thru_hole oval
			(at 25.4 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(A1-D4-Pad19)")
			(pinfunction "D4")
			(pintype "bidirectional")
			(uuid "407b532e-3b37-4c06-aa37-fdefbf6621fd")
		)
		(pad "20" thru_hole oval
			(at 22.86 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-D5-Pad20)")
			(pinfunction "D5")
			(pintype "bidirectional")
			(uuid "a49ac29e-ef9c-4e66-b6b7-9a46fa69f2c9")
		)
		(pad "21" thru_hole oval
			(at 20.32 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(A1-D6-Pad21)")
			(pinfunction "D6")
			(pintype "bidirectional")
			(uuid "99a35560-d17d-490e-a471-63606b2c6327")
		)
		(pad "22" thru_hole oval
			(at 17.78 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(A1-D7-Pad22)")
			(pinfunction "D7")
			(pintype "bidirectional")
			(uuid "68a5ccb5-2ef5-4c69-b22a-ce0c6e207fd9")
		)
		(pad "23" thru_hole oval
			(at 13.72 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(A1-D8-Pad23)")
			(pinfunction "D8")
			(pintype "bidirectional")
			(uuid "e2ceb61d-5ae2-4bc7-9f07-c2c213fcae54")
		)
		(pad "24" thru_hole oval
			(at 11.18 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(A1-D9-Pad24)")
			(pinfunction "D9")
			(pintype "bidirectional")
			(uuid "50ed5478-3fba-4a3a-844c-999d2606d847")
		)
		(pad "25" thru_hole oval
			(at 8.64 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(A1-D10-Pad25)")
			(pinfunction "D10")
			(pintype "bidirectional")
			(uuid "d3b05d77-2b7c-45d7-962d-22ed820d6c07")
		)
		(pad "26" thru_hole oval
			(at 6.1 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-D11-Pad26)")
			(pinfunction "D11")
			(pintype "bidirectional")
			(uuid "c93ebdca-34d2-4217-b57c-14deaef1cab1")
		)
		(pad "27" thru_hole oval
			(at 3.56 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(A1-D12-Pad27)")
			(pinfunction "D12")
			(pintype "bidirectional")
			(uuid "ee5eb015-9b79-42b0-8bb8-85f11cc0cbd3")
		)
		(pad "28" thru_hole oval
			(at 1.02 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(A1-D13-Pad28)")
			(pinfunction "D13")
			(pintype "bidirectional")
			(uuid "38429ed2-e5c0-4a19-a1d7-9f216519eea1")
		)
		(pad "29" thru_hole oval
			(at -1.52 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D1-K)")
			(pinfunction "GND")
			(pintype "power_in")
			(uuid "6cc9ceaa-6f41-4d11-a42b-d221c2c20b8a")
		)
		(pad "30" thru_hole oval
			(at -4.06 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(A1-AREF-Pad30)")
			(pinfunction "AREF")
			(pintype "input")
			(uuid "52d63ddd-41a4-49f2-9180-a728bf48e790")
		)
		(pad "31" thru_hole oval
			(at -6.6 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-SDA{slash}A4-Pad31)")
			(pinfunction "SDA/A4")
			(pintype "bidirectional")
			(uuid "82729b22-3648-4fa2-aff6-030e54a44d5a")
		)
		(pad "32" thru_hole oval
			(at -9.14 48.26 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(A1-SCL{slash}A5-Pad32)")
			(pinfunction "SCL/A5")
			(pintype "bidirectional")
			(uuid "b478cbc0-576c-43b9-ad39-a1b166f5a6f6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Arduino_UNO_R3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(uuid "e2d848fd-f34a-44b2-b9d9-dff3b4128436")
		(at 169.845 137 180)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 3.655 1.5 0)
			(layer "F.SilkS")
			(uuid "f1985cd1-fdd6-424b-8440-04d438db3d7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.05 0)
			(layer "F.Fab")
			(uuid "7260cd2e-3823-4687-bf51-6b397294b1db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "83d2c70a-4b93-48c8-a595-f19623e3c76a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "be7b8886-b9b7-489c-8d5b-933d31499db3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f584e00a-94cf-4f9d-9165-dc564586e2dd")
		(sheetname "/")
		(sheetfile "03_KiCad_simpleLED.kicad_sch")
		(attr smd)
		(fp_rect
			(start -0.7 -0.35)
			(end 0.7 0.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "590080e4-2c82-44c4-82b8-340a0ee14b2f")
		)
		(fp_rect
			(start -0.3 -0.15)
			(end 0.3 0.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8c757f32-d1ae-42ba-b479-01312e7b41e8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
			(uuid "04378f01-5cc1-48ab-a72c-06142b32ecbb")
			(effects
				(font
					(size 0.25 0.25)
					(thickness 0.04)
				)
			)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "4745cb0f-37ad-4e09-8bf0-0a1353fde78e")
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(uuid "023edac8-0bdf-4ed3-9622-eb86201cb146")
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(A1-D2)")
			(pintype "passive")
			(uuid "2f0482ab-b99d-4b55-80e7-f6d7a8d01472")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(D1-A)")
			(pintype "passive")
			(uuid "a2826c9d-6b5e-4e07-9c4a-b56401347188")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 100.5 54.5)
		(end 191 148)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "d03d8cf7-3f3d-4259-b725-152180f88b9a")
	)
	(segment
		(start 170.805 128.63)
		(end 170.805 136.36)
		(width 0.2)
		(layer "F.Cu")
		(net 12)
		(uuid "c71378ce-2ee9-4530-87f8-31c781c26e85")
	)
	(segment
		(start 170.805 136.36)
		(end 170.165 137)
		(width 0.2)
		(layer "F.Cu")
		(net 12)
		(uuid "d9a56101-c6b1-45b8-a5d8-7431b2b6499e")
	)
	(segment
		(start 138.805 136.805)
		(end 139 137)
		(width 0.2)
		(layer "F.Cu")
		(net 14)
		(uuid "a4bb6ac8-a5f2-4c81-b729-1ab5e3ba4b25")
	)
	(segment
		(start 138.805 128.63)
		(end 138.805 136.805)
		(width 0.2)
		(layer "F.Cu")
		(net 14)
		(uuid "eb4121e5-4d61-4820-a304-886d5b0e5bcc")
	)
	(segment
		(start 153.025 69.125)
		(end 153.025 80.37)
		(width 0.2)
		(layer "F.Cu")
		(net 22)
		(uuid "5e49ce59-3feb-40d9-b477-5d55d4fc471b")
	)
	(segment
		(start 149.5 65.6)
		(end 153.025 69.125)
		(width 0.2)
		(layer "F.Cu")
		(net 22)
		(uuid "88e7a25e-fcad-4fec-ab72-64e549977471")
	)
	(segment
		(start 158.105 80.37)
		(end 165.275 73.2)
		(width 0.2)
		(layer "F.Cu")
		(net 23)
		(uuid "ce74f2f8-2584-4609-a50e-2418b713ea65")
	)
	(segment
		(start 165.275 73.2)
		(end 169.5 73.2)
		(width 0.2)
		(layer "F.Cu")
		(net 23)
		(uuid "e75997af-99cc-404b-a555-c4603ad6f120")
	)
	(segment
		(start 161.9 58)
		(end 149.5 58)
		(width 0.2)
		(layer "F.Cu")
		(net 33)
		(uuid "9abf0bb0-e99b-4488-bad0-58b95661c47a")
	)
	(segment
		(start 169.5 65.6)
		(end 161.9 58)
		(width 0.2)
		(layer "F.Cu")
		(net 33)
		(uuid "ca616574-1fe8-4816-b77b-add60b415b39")
	)
	(segment
		(start 139.665 137)
		(end 169.525 137)
		(width 0.2)
		(layer "F.Cu")
		(net 34)
		(uuid "bc3398ad-f9f9-4d82-95ae-78b80f0d9fb1")
	)
	(embedded_fonts no)
)
