<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LONGPADS">
</package>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="01_adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="01_SparkFun" package="1X02_LONGPADS" value=""/>
<element name="LED1" library="01_adafruit" package="CHIP-LED0603" value=""/>
<element name="LED2" library="01_adafruit" package="CHIP-LED0603" value=""/>
<element name="LED3" library="01_adafruit" package="CHIP-LED0603" value=""/>
<element name="LED4" library="01_adafruit" package="CHIP-LED0603" value=""/>
<element name="LED5" library="01_adafruit" package="CHIP-LED0603" value=""/>
<element name="R1" library="01_adafruit" package="M0805" value="10k"/>
<element name="R2" library="01_adafruit" package="M0805" value="200"/>
<element name="U$1" library="01_SparkFun" package="SO08-EIAJ" value="ATTINY45"/>
<element name="U$2" library="01_fab" package="2X03SMD" value="AVRISPSMD"/>
</elements>
<signals>
<signal name="N$4">
<contactref element="LED1" pad="A"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="7"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="PB1">
<contactref element="U$2" pad="1"/>
<contactref element="LED4" pad="A"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="4"/>
<contactref element="LED5" pad="A"/>
<contactref element="U$1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
