<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<text>LilyF</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="C1206FAB">
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="TQFP32-08THIN">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="LilyPad-Wearables">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of sewable boards, textile footprints, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SIMPLE_HOLE">
</package>
<package name="LED-1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="fab" package="R1206W" value="10K"/>
<element name="C1" library="fab" package="C1206FAB" value="4uF"/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$3" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="H1" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H2" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H3" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H4" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H5" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="VCC" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H7" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="GND" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H8" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="H9" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="R2" library="fab" package="R1206FAB" value="330"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="C2" library="fab" package="C1206" value="1.0uF"/>
<element name="LED1" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="C3" library="fab" package="C1206" value="0.1 uF"/>
<element name="C4" library="fab" package="C1206" value="0.1uF"/>
<element name="R3" library="fab" package="R1206FAB" value="0"/>
<element name="H10" library="LilyPad-Wearables" package="SIMPLE_HOLE" value="SEW_HOLE"/>
<element name="IC1" library="fab" package="TQFP32-08THIN" value="ATMEGA88-THIN"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$3" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="18"/>
<contactref element="VCC" pad="P$1"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="17"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="5"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$1">
</signal>
<signal name="RXD">
<contactref element="U$3" pad="5"/>
</signal>
<signal name="TXD">
<contactref element="U$3" pad="4"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="RTS">
<contactref element="C4" pad="1"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="21"/>
<contactref element="GND" pad="P$1"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="23"/>
<contactref element="H3" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="25"/>
<contactref element="H5" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="28"/>
<contactref element="H8" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="32"/>
<contactref element="H4" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="1"/>
<contactref element="H1" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="2"/>
<contactref element="H2" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="9"/>
<contactref element="H9" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="11"/>
<contactref element="H10" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="22"/>
<contactref element="H7" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
