<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<text>  Level 
Converter</text>
<text>Nathan Seidle</text>
<text>Rev V13 by Patrick Alberts</text>
<text>HV1</text>
<text>HV2</text>
<text>HV</text>
<text>GND</text>
<text>HV3</text>
<text>HV4</text>
<text>LV1</text>
<text>LV4</text>
<text>LV3</text>
<text>LV2</text>
<text>LV</text>
<text>GND</text>
<text>HV1</text>
<text>HV4</text>
<text>HV2</text>
<text>HV3</text>
<text>GND</text>
<text>GND</text>
<text>HV</text>
<text>LV</text>
<text>LV3</text>
<text>LV2</text>
<text>LV4</text>
<text>LV1</text>
<text>MD</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SOT23-3">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SFE_LOGO_FLAME_.1">
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA05-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="PANASONIC_D">
</package>
</packages>
</library>
<library name="01_FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q2" library="SparkFun" package="SOT23-3" value="BSS138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="SparkFun" package="SOT23-3" value="BSS138"/>
<element name="R1" library="SparkFun" package="0603-RES" value="10K"/>
<element name="R5" library="SparkFun" package="0603-RES" value="10K"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="SFE_LOGO_FLAME_.1" value="SFE_LOGO_FLAME.1_INCH"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="SV1" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SV2" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="IC1" library="01_SparkFun" package="SOT223" value=""/>
<element name="C1" library="01_SparkFun" package="PANASONIC_D" value=""/>
<element name="C2" library="01_SparkFun" package="PANASONIC_D" value=""/>
<element name="TEMPSENS" library="con-lstb" package="MA03-1" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="RGB" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R2" library="01_FAB_Hello" package="1206" value=""/>
<element name="R3" library="01_FAB_Hello" package="1206" value=""/>
<element name="R4" library="01_FAB_Hello" package="1206" value=""/>
<element name="ACCBTN" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R8" library="01_FAB_Hello" package="1206" value=""/>
<element name="TOBOARD" library="con-lstb" package="MA05-1" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="R9" library="01_FAB_Hello" package="1206" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="SV1" pad="4"/>
<contactref element="SV2" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="LV">
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="ACCBTN" pad="4"/>
</signal>
<signal name="HV">
<contactref element="R7" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="SV2" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="+"/>
<contactref element="TEMPSENS" pad="1"/>
<contactref element="ACCBTN" pad="2"/>
<contactref element="RGB" pad="1"/>
</signal>
<signal name="LV4">
<contactref element="Q2" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="LV3">
<contactref element="Q4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="HV3">
<contactref element="Q4" pad="3"/>
<contactref element="R5" pad="2"/>
<contactref element="SV2" pad="3"/>
</signal>
<signal name="HV4">
<contactref element="Q2" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="TEMP">
<contactref element="TEMPSENS" pad="2"/>
<contactref element="TOBOARD" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="RGB" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="RGB" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="L1">
<contactref element="R2" pad="2"/>
<contactref element="TOBOARD" pad="5"/>
</signal>
<signal name="L2">
<contactref element="R3" pad="2"/>
<contactref element="TOBOARD" pad="4"/>
</signal>
<signal name="L3">
<contactref element="R4" pad="2"/>
<contactref element="TOBOARD" pad="3"/>
</signal>
<signal name="BTN">
<contactref element="TOBOARD" pad="2"/>
<contactref element="ACCBTN" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="TEMPSENS" pad="3"/>
<contactref element="R9" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="ACCBTN" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="RGB" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
