<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="1X04-SMD">
</package>
<package name="SWITCH-SPDT-SMD">
</package>
<package name="1X01_LONGPAD">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="TQFP32-08THIN">
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="01_adafruit">
<packages>
<package name="JST-PH-2-SMT">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="01_SparkFun" package="1206" value="499"/>
<element name="R10" library="01_SparkFun" package="1206" value="499"/>
<element name="R2" library="01_SparkFun" package="1206" value="499"/>
<element name="R3" library="01_SparkFun" package="1206" value="499"/>
<element name="R4" library="01_SparkFun" package="1206" value="499"/>
<element name="R5" library="01_SparkFun" package="1206" value="499"/>
<element name="R6" library="01_SparkFun" package="1206" value="499"/>
<element name="R7" library="01_SparkFun" package="1206" value="499"/>
<element name="R8" library="01_SparkFun" package="1206" value="499"/>
<element name="R9" library="01_SparkFun" package="1206" value="499"/>
<element name="S1" library="01_ng" package="6MM_SWITCH" value=""/>
<element name="T1" library="01_fab" package="SOT-23" value=""/>
<element name="T2" library="01_fab" package="SOT-23" value=""/>
<element name="T3" library="01_fab" package="SOT-23" value=""/>
<element name="CN1" library="01_adafruit" package="JST-PH-2-SMT" value=""/>
<element name="HC-SR04" library="01_SparkFun" package="1X04-SMD" value=""/>
<element name="S2" library="01_SparkFun" package="SWITCH-SPDT-SMD" value=""/>
<element name="R11" library="01_SparkFun" package="1206" value="10k"/>
<element name="JP1" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP2" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP3" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP4" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP5" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP6" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP7" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP8" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP9" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP10" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP11" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP12" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP13" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="U$1" library="01_fab" package="TQFP32-08THIN" value="ATMEGA88-THIN"/>
<element name="JP14" library="01_fab" package="2X03SMD" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R11" pad="2"/>
<contactref element="HC-SR04" pad="4"/>
<contactref element="CN1" pad="2"/>
<contactref element="JP14" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="20"/>
<contactref element="U$1" pad="18"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="29"/>
<contactref element="R11" pad="1"/>
<contactref element="JP14" pad="5"/>
</signal>
<signal name="BUTTON">
<contactref element="S1" pad="1"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="GND">
<contactref element="HC-SR04" pad="1"/>
<contactref element="CN1" pad="1"/>
<contactref element="JP14" pad="6"/>
<contactref element="T1" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="T3" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="21"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="ECHO">
<contactref element="HC-SR04" pad="2"/>
<contactref element="U$1" pad="31"/>
</signal>
<signal name="TRIG">
<contactref element="HC-SR04" pad="3"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R3" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R4" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R5" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R6" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R7" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R8" pad="2"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R9" pad="2"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R10" pad="2"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="COL4">
<contactref element="U$1" pad="15"/>
<contactref element="JP14" pad="4"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="COL3">
<contactref element="U$1" pad="14"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="COL2">
<contactref element="U$1" pad="13"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="COL1">
<contactref element="U$1" pad="12"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="ROW3">
<contactref element="U$1" pad="11"/>
<contactref element="T3" pad="3"/>
</signal>
<signal name="ROW2">
<contactref element="U$1" pad="10"/>
<contactref element="T2" pad="3"/>
</signal>
<signal name="ROW1">
<contactref element="U$1" pad="9"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="COL9">
<contactref element="U$1" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="U$1" pad="19"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="28"/>
</signal>
<signal name="N$39">
<contactref element="U$1" pad="27"/>
</signal>
<signal name="N$40">
<contactref element="U$1" pad="26"/>
</signal>
<signal name="N$41">
<contactref element="U$1" pad="25"/>
</signal>
<signal name="N$43">
<contactref element="U$1" pad="23"/>
</signal>
<signal name="COL6">
<contactref element="U$1" pad="17"/>
<contactref element="JP14" pad="3"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="COL5">
<contactref element="U$1" pad="16"/>
<contactref element="JP14" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="COL10">
<contactref element="U$1" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="24"/>
</signal>
<signal name="N$34">
<contactref element="JP11" pad="1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="JP12" pad="1"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="JP13" pad="1"/>
<contactref element="T3" pad="1"/>
</signal>
<signal name="COL8">
<contactref element="U$1" pad="8"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="COL7">
<contactref element="U$1" pad="7"/>
<contactref element="R7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
