<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="33.01" width="0" layer="20"/>
<wire x1="100" y1="33.01" x2="0" y2="33.01" width="0" layer="20"/>
<wire x1="0" y1="33.01" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
<library name="01_adafruit">
<packages>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="01_SparkFun" package="1X06-SMD" value=""/>
<element name="LED1" library="01_adafruit" package="1206" value=""/>
<element name="LED5" library="01_adafruit" package="1206" value=""/>
<element name="LED15" library="01_adafruit" package="1206" value=""/>
<element name="LED23" library="01_adafruit" package="1206" value=""/>
<element name="LED7" library="01_adafruit" package="1206" value=""/>
<element name="LED17" library="01_adafruit" package="1206" value=""/>
<element name="LED9" library="01_adafruit" package="1206" value=""/>
<element name="LED2" library="01_adafruit" package="1206" value=""/>
<element name="LED12" library="01_adafruit" package="1206" value=""/>
<element name="LED20" library="01_adafruit" package="1206" value=""/>
<element name="LED26" library="01_adafruit" package="1206" value=""/>
<element name="LED11" library="01_adafruit" package="1206" value=""/>
<element name="LED28" library="01_adafruit" package="1206" value=""/>
<element name="LED22" library="01_adafruit" package="1206" value=""/>
<element name="LED14" library="01_adafruit" package="1206" value=""/>
<element name="LED4" library="01_adafruit" package="1206" value=""/>
<element name="LED6" library="01_adafruit" package="1206" value=""/>
<element name="LED16" library="01_adafruit" package="1206" value=""/>
<element name="LED24" library="01_adafruit" package="1206" value=""/>
<element name="LED18" library="01_adafruit" package="1206" value=""/>
<element name="LED8" library="01_adafruit" package="1206" value=""/>
<element name="LED10" library="01_adafruit" package="1206" value=""/>
<element name="LED19" library="01_adafruit" package="1206" value=""/>
<element name="LED30" library="01_adafruit" package="1206" value=""/>
<element name="LED25" library="01_adafruit" package="1206" value=""/>
<element name="LED29" library="01_adafruit" package="1206" value=""/>
<element name="LED3" library="01_adafruit" package="1206" value=""/>
<element name="LED13" library="01_adafruit" package="1206" value=""/>
<element name="LED21" library="01_adafruit" package="1206" value=""/>
<element name="LED27" library="01_adafruit" package="1206" value=""/>
</elements>
<signals>
<signal name="N$26">
<contactref element="LED18" pad="C"/>
<contactref element="LED17" pad="A"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED20" pad="A"/>
<contactref element="LED21" pad="C"/>
<contactref element="LED22" pad="A"/>
<contactref element="LED23" pad="C"/>
<contactref element="LED24" pad="A"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED8" pad="C"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$31">
<contactref element="LED11" pad="C"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED13" pad="C"/>
<contactref element="LED14" pad="A"/>
<contactref element="LED15" pad="C"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED17" pad="C"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED10" pad="C"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="A"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED10" pad="A"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="LED30" pad="C"/>
<contactref element="LED29" pad="A"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED19" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED20" pad="C"/>
<contactref element="LED25" pad="A"/>
<contactref element="LED26" pad="C"/>
<contactref element="LED1" pad="A"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="LED28" pad="C"/>
<contactref element="LED27" pad="A"/>
<contactref element="LED30" pad="A"/>
<contactref element="LED29" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED21" pad="A"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED14" pad="C"/>
<contactref element="LED22" pad="C"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="LED24" pad="C"/>
<contactref element="LED23" pad="A"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED26" pad="A"/>
<contactref element="LED25" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED28" pad="A"/>
<contactref element="LED27" pad="C"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$11">
</signal>
</signals>
</board>
</drawing>
</eagle>
