<!--This work is licensed under a Creative Commons Attribution-ShareAlike 4.0 International License (CC BY-SA) with Design Exception 1.0-->
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="DPAK228P968X238-4N">
</package>
</packages>
<symbols>
<symbol name="NJM2845DL1-33-TE1">
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NJM2845DL1-33-TE1" prefix="U">
<description>NJM2845 Series 800 mA 3.3 V Fixed Output SMT LDO Regulator - TO-252</description>
<gates>
<gate name="G$1" symbol="NJM2845DL1-33-TE1"/>
</gates>
<devices>
<device name="" package="DPAK228P968X238-4N">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="Availability" value="Unavailable"/>
<attribute name="Price" value="None"/>
<attribute name="Description" value="
Linear Voltage Regulator IC 1 Output 800mA TO-252-3
"/>
<attribute name="Package" value="TO-252-3 New Japan Radio"/>
<attribute name="MP" value="NJM2845DL1-33-TE1"/>
<attribute name="MF" value="NJR Corporation/NJRC"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
