MATERIALS

Wood - 3mm
For two round plates (middle and bottom)
600x300mm

Transparent acrylic - 3mm
Round top plate
300x300mm

Acrylic Tan - 6mm
For spaces and active gears
150 x 300 mm

Acrylic Tan - 3mm
For decorative gears
150 x 100mm

Acrylic Tube Transparent - 5mm diameter 
For cam shaft stops
4x 3mm
plus a 1.5mm drill

Copperplated shaft - 3mm diameter
For hinges between bug and wings
2x 30 mm
plus threading tools for M3

Copperplated shaft - 4mm diameter
For fastening the plates together 
6x 36 mm
plus threading tools for M4

Nuts & bolts

For gears:
4x M3 40 mm flat head

For motor:
2x M3 9mm flat head bolts
2x M3 nuts
2x M3 washers 

Fastening:
9x M3 Brass capped nuts (for hinge, gears)
12x M4 Brass capped nuts (for fastening plates together)

Cam shafts
200 mm long - 1,5mm copper plated wire

3D print filament for uPrint printer (ABS)
Model material: 41,14 cm3
Support material: 30,96 cm3
Citric acid wash to dissolve support: 1 bag
Printing time: 8 hrs

Adhesives
Acrifix thick - 1R 0192
Loctite 270
Bison hard plastic glue

Electronics parts 
50 x70 mm copper plated PCB board - doublesided
2x 6 pin connector (2x3)
jumper wires
Solder
5V FTDI cable for programming
DC supply

Part          Value            Package           Library             Position (mm)         Orientation

5V_REG      LM2940IMP-5.0    SOT230P696X180-4N 01Texas_5Vregulator (20.49 15.25)         R90
BULB1         3.5V             LED5MM            led                 (8.25 36.6)           R0 
	>> foot print for: incandescent bulbs 3.5V, 0.2A > http://nl.opitec.com/opitec-web/articleNumber/202019/zz/cID/c3I6bGFtcGplczI=
BULB2         3.5V             LED5MM            led                 (15.7 36.6)           R0
	>> foot print for: incandescent bulbs 3.5V, 0.2A > http://nl.opitec.com/opitec-web/articleNumber/202019/zz/cID/c3I6bGFtcGplczI=
JP1           FTDI_BASICPTH    FTDI_BASIC        SparkFun-Connectors (61.97 31.14)         R270
MIC_THRU      electret         1X02              pinhead             (42.53 37.74)         R270
	>> footprint for : MIC      ELECTRET_MICROPHON-WM-61A WM-61A              01_echo_mic  (1.64 18.14)          R0
MOTOR    UNIPOLAR         2X03SMD           01_fab              (56.35 8.7)           R270
	>> footprint for : Nippon Pulse Unipolar Stepper PF35T-48L4
SUPPLY   1X2-3.5MM SUPPLY 3.5MMTERM         01_adafruit         (8.95 8.4)            R90
SWITCH   1X2-3.5MM SUPPLY 3.5MMTERM         01_adafruit         (8.94 20.83)          R90
6pin hdr	AVRISP           2X03SMD           01_fab              (38.43 9.3)           R270
C1            1uF              1206              01_FAB_Hello        (35.46 39.37)         R180
C4            1nF              1206              01_FAB_Hello        (36.17 31.95)         R180
C5            0.47uF (470nF)   1206              01_FAB_Hello        (16.47 23.33)         R0
	> 1uF instead
C6            30uF             1206              01_FAB_Hello        (19.95 7.05)          R0
	> 3x 10uF on top of one another (stack in series)
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R2            10 ohm           1206              01_FAB_Hello        (54.15 38.6)          R270
R12          10K              1206              01_FAB_Hello        (15.7 29.3)           R90
R13          10K              1206              01_FAB_Hello        (24.8 35.6)           R90
R14          10K              1206              01_FAB_Hello        (22.6 39.4)           R180
R15          10K              1206              01_FAB_Hello        (20.2 35.55)          R90
R16          10K              1206              01_FAB_Hello        (22.5 35.55)          R90
R1            1K               1206              01_FAB_Hello        (49.04 38.45)         R270
IC1           ATTINY84         SOIC14            001fab              (36.72 22.96)         R270
T1            1.7A             SOT-23            001fab              (54.2 20.95)          R90
T2            1.7A             SOT-23            001fab              (54.95 30.55)         R90
T3            1.7A             SOT-23            001fab              (47.65 14.8)          R90
T4            1.7A             SOT-23            001fab              (48 25.85)            R90
T5            NMOS             SOT-23            001fab              (6.3 29.65)           R90
T6            NMOS             SOT-23            001fab              (24.55 25.7)          R90
SCHOTTKYDIODE 100V/1A          SOD-123H          01comchip           (8.89 14.53)          R180
IC2           OPAMP            SOT23-5           01_ng               (61.5 39.1)           R0