<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.61" y2="0" width="0" layer="20"/>
<wire x1="27.61" y1="0" x2="27.61" y2="40.63" width="0" layer="20"/>
<wire x1="27.61" y1="40.63" x2="0" y2="40.63" width="0" layer="20"/>
<wire x1="0" y1="40.63" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="A3216-18">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Wave solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
</packages>
</library>
<library name="01_fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="01_SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_LONGPAD">
</package>
<package name="S2B-PH">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="SWITCH-SPDT-SMD">
</package>
<package name="VIBE-MOTOR-10MM">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="01_ng">
<description>Neil Gershenfeld's library</description>
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="ng" package="A3216-18" value="1uF"/>
<element name="IC1" library="01_fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="JP1" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP10" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP11" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP12" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP13" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP14" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP15" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP2" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP3" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP4" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP5" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP6" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="JP7" library="01_SparkFun" package="S2B-PH" value=""/>
<element name="JP8" library="01_SparkFun" package="1X01_LONGPAD" value="M01PTH_LONGPAD"/>
<element name="R1" library="01_ng" package="1206" value="499"/>
<element name="R2" library="01_ng" package="1206" value="499"/>
<element name="R3" library="01_ng" package="1206" value="499"/>
<element name="R4" library="01_ng" package="1206" value="499"/>
<element name="R5" library="01_ng" package="1206" value="499"/>
<element name="R6" library="01_ng" package="1206" value="499"/>
<element name="R7" library="01_ng" package="1206" value="10k"/>
<element name="S1" library="01_fab" package="6MM_SWITCH" value=""/>
<element name="S2" library="01_fab" package="6MM_SWITCH" value=""/>
<element name="S5" library="01_SparkFun" package="SWITCH-SPDT-SMD" value=""/>
<element name="T1" library="01_ng" package="SOT-23" value=""/>
<element name="U$5" library="01_SparkFun" package="VIBE-MOTOR-10MM" value="MOTOR10MM"/>
<element name="JP9" library="01_SparkFun" package="1X01" value="M01PTH"/>
<element name="JP16" library="01_SparkFun" package="1X01" value="M01PTH"/>
<element name="JP17" library="01_SparkFun" package="1X01" value="M01PTH"/>
<element name="JP18" library="01_SparkFun" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="LED1">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="LED2">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="LED3">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="LED4">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="LED5">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="MOSI">
<contactref element="JP11" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="JP10" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="JP14" pad="1"/>
<contactref element="IC1" pad="9"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="-"/>
<contactref element="JP13" pad="1"/>
<contactref element="T1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="JP8" pad="1"/>
<contactref element="S5" pad="3"/>
</signal>
<signal name="RST">
<contactref element="JP15" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R7" pad="2"/>
<contactref element="JP12" pad="1"/>
<contactref element="C1" pad="+"/>
<contactref element="U$5" pad="-"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U$5" pad="+"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="MOTOR">
<contactref element="IC1" pad="6"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="BUTTA">
<contactref element="IC1" pad="12"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="BUTTB">
<contactref element="IC1" pad="13"/>
<contactref element="S2" pad="4"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="JP7" pad="1"/>
<contactref element="S5" pad="2"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
